{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","ADEA71A2VEB / AZAS71M2V1B","ADEA100A2VEB / AZAS100M7V1B","ADEA125A2VEB / AZAS125M7V1B"]
["Outdoor unit","","","","AZAS71M2V1B","AZAS100M7V1B","AZAS125M7V1B"]
["Cooling capacity","Nom.","","kW","6.80","9.50","12.10"]
["Heating capacity","Nom.","","kW","7.50","10.80","13.50"]
["Nominal efficiency","EER","","","3.27","3.20","2.27"]
["","COP","","","3.62","4.63","3.89"]
["Space cooling","Energy efficiency class","","","A","A"]
["","Capacity","Pdesign","kW","6.80","9.50","12.10"]
["","SEER","","","5.44","5.13","4.73"]
["","Annual energy consumption","","kWh/a","437","648","1534"]
["Space heating (Average climate)","Energy efficiency class","","","A","A"]
["","Capacity","Pdesign","kW","4.50","6.00","6.00"]
["","SCOP/A","","","3.81","3.81","3.50"]
["","Pdh Heating capacity at -10°","","kW","4.50","6.00","6.00"]
["","Annual energy consumption","","kWh/a","1654","2206","2399"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]