{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":11,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C"]
[]
[]
[]
[]
["","","","","","ADEQ35C2VEB","ADEQ50C2VEB","ADEQ60C2VEB","ADEQ71C2VEB","ADEQ100C2VEB","ADEQ125C2VEB"]
["Fan","External static pressure","","High","Pa","150","150","150","150","150","150"]
["Cooling capacity","Total capacity","","Nom.","kW","","","","","","12.10"]
["Heating capacity","Total capacity","","Nom.","kW","","","","","","13.5"]
["Casing","Colour","","","","Unpainted","Unpainted","Unpainted","Unpainted","Unpainted","Unpainted"]
["","Material","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["Dimensions","Unit","","Height","mm","245","245","245","245","245","245"]
["","","","Width","mm","700","700","1000","1000","1400","1400"]
["","","","Depth","mm","800","800","800","800","800","800"]
["Weight","Unit","","","kg","28","28","35","35","46","46"]
["Fan","Air flow rate","Cooling","High","m³/min","15","15","18","18","29","34"]
["","","","Nom.","m³/min","15.0","15.0","18.0","18.0","29.0","34.0"]
["","","","Medium","m³/min","12.5","12.5","15","15","26","29"]
["","","","Low","m³/min","10.5","10.5","12.5","12.5","23","23.5"]
["","","Heating","High","m³/min","15","15","18","18","29","34"]
["","","","Nom.","m³/min","15.0","15.0","18.0","18.0","29.0","34.0"]
["","","","Medium","m³/min","12.5","12.5","15","15","26","29"]
["","","","Low","m³/min","10.5","10.5","12.5","12.5","23","23.5"]
["","External static pressure","","Nom.","Pa","30","30","30","30","40","50"]
["Sound power level","Cooling","","","dBA","60","60","56","56","58","62"]
["Sound pressure level","Cooling","","High","dBA","35","35","30","30","34","37"]
["","","","Nom.","dBA","35","35","30","30","34","37"]
["","","","Medium","dBA","32","32","28","28","32","35"]
["","","","Low","dBA","29","29","25","25","30","32"]
["","Heating","","High","dBA","37","37","31","31","36","38"]
["","","","Medium","dBA","34","34","28","28","33","35"]
["","","","Nom.","dBA","37","37","31","31","36","38"]
["","","","Low","dBA","29","29","25","25","30","32"]
["Refrigerant","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","9.52","9.52","9.52"]
["","Gas","","OD","mm","9.52","12.7","12.7","15.9","15.9","15.9"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8","8","8"]
["","Operation manual","","","","1","1","1","1","1","1"]
["","Clamps","","","","4","4","4","4","4","4"]
["","Drain hose","","","","1","1","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","1","1","1"]
["","Screws","","","","40","40","40","40","40","40"]
["","Sealing pad","","","","5","5","5","5","5","5"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates.","(1) - The sound power level is an absolute value indicating the power which a sound source generates."]