{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXF-F"]
[]
[]
[]
[]
["","","","","","ARXF20F5V1B","ARXF25F5V1B","ARXF35F5V1B","ARXF42F5V1B","ARXF50F5V1B"]
["Dimensions","Unit","","Height","mm","556","556","556","556","610"]
["","","","Width","mm","740","740","740","740","923"]
["","","","Depth","mm","343","343","343","343","367"]
["Weight","Unit","","","kg","24","24","24","28","40.0"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","-10","-10","-10","-10"]
["","","","Max.","°CDB","48","48","48","48","48"]
["","Heating","Ambient","Min.","°CWB","-15","-15","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18","18","18"]
["Sound pressure level","Cooling","","High","dBA","46","46","48","48","48.0"]
["","Heating","","High","dBA","47","47","48","48","49.0"]
["Refrigerant","Type","","","","R-32","R-32","R-32","R-32","R-32"]
["","Charge","","","kg","0.42","0.42","0.55","0.75","0.800"]
["","Charge","","","tCO2Eq","0.28","0.28","0.37","0.51","0.540"]
["","GWP","","","","675","675","675","675","675.0"]
["Piping connections","Piping length","OU - IU","Max.","m","20","20","20","20","30"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02"]
["","Level difference","IU - OU","Max.","m","12","12","12","12","20.0"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1"]
["","Drain plug","","","","1","1","1","1"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases"]
["","","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]