{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":22,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AS"]
[]
[]
[]
[]
["","","","","","MAS121T1000E","MAS123T1000E","MAS121T443S","MAS221N1000E","MAS221N443S","MAS221T1000E","MAS123T443S","BAS135T02Y","MAS235T02E","MAS235T1000E","MAS135N02Y","MAS135T02Y","MAS135T1000E","MAS335N02E","MAS335N1000E","MAS335T02E","MAS340T02E"]
["Refrigerant","GWP","","","","1,430","1,430","1,774","1,430","1,774","1,430","1,774","3.0","1,430","1,430","3.0","3.0","1,430","1,430","1,430","1,430","1,430"]
["","Type","","","","R-134a","R-134a","R-407C","R-134a","R-407C","R-134a","R-407C","R-290","R-134a","R-134a","R-290","R-290","R-134a","R-134a","R-134a","R-134a","R-134a"]
["Refrigerating capacity","Medium temperature","R-134a","Nom","kW","1.140","1.422","","1.816","","2.029","","","4.981 (1)","4.981","","","3.492","6.988 (1)","6.988","8.290 (1)","10.664 (1)"]
["","","R-290","Nom","kW","","","","","","","","","","","2.614 (1)","3.479 (1)"]
["","Low temperature","R-290","Nom","kW","","","","","","","","2.789 (1)"]
["Operation range","Cold room temperature","","Min.","°C","","","0","","0","","0","","-5","","","","","-5","","-5","-5"]
["","","","Max.","°C","","","15","","15","","15","","10","","","","","10","","10","10"]
["Defrost","","","","","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas","","Hot gas","Hot gas","","","Hot gas","Hot gas","Hot gas","Hot gas","Hot gas"]
["Dimensions","Unit","","Width","mm","537","537","537","832","832","832","537","900","1,280","1,329","900","900","832","1,750","1,766","1,750","1,790"]
["","","","Depth","mm","825","825","825","825","825","825","825","1,170","1,140","1,140","1,170","1,170","1,100","1,140","1,140","1,140","1,240"]
["","","","Height","mm","705","705","705","695","695","695","705","800","857","690","800","800","800","857","690","857","857"]
["Compressor","Nominal power","","","kW","0.6","0.74","0.46","0.9","0.74","1.1","0.56","","3.7","3.7","","","2.6","4.8","4.8","6.3","7.4"]
["","Type","","","","Hermetic","Hermetic","Hermetic","Hermetic","Hermetic","Hermetic","Hermetic","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic","Hermetic Reciprocating","Hermetic","Hermetic Reciprocating","Hermetic Reciprocating"]
["","Starting method","","","","Direct","Direct","Direct","Direct","Direct","Direct","Direct","","Direct","Direct","","","Direct","Direct","Direct","Direct","Direct"]
["Weight","Unit","","","kg","53","57","53","77","77","79","57","106","162","162","106","106","104","221","217","222","244"]
["Condenser","Air flow","","","m³/h","","","700","","1,400","","700","","2,700","","","","","4,000","","4,000","5,600"]
["Evaporator","Air flow","","","m³/h","","","600","","1,200","","600","","3,900","","","","","5,600","","5,600","8,000"]
["","Air throw","","","m","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","","10 (2)","10 (2)","","","10 (2)","10 (2)","10 (2)","10 (2)","17 (2)"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","3N~","1~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","230","230","230","230","230","400","230","400","400","400","400","400","400","400","400","400","400"]
["Notes","","","","","","","","","","","","(1) - Contains fluorinated greenhouse gases","","","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases"]
["","","","","","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","","","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C"]
["","","","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc."]
["","","","","","","","","","","","","","(3) - Contains fluorinated greenhouse gases","","","","","(3) - Contains fluorinated greenhouse gases","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases"]