{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":80,"n_cols":11,"rows_kept":80,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF25A5V1B","ATXF35A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B"]
["Sound pressure level","Heating","","High","dBA","40","","","42","44","45"]
["","","","Medium","dBA","34","","","38","40","41"]
["","","","Silent operation","dBA","21","","","30","32","33"]
["","","","Low","dBA","28","","","33","35","36"]
["","Cooling","","Medium","dBA","33","","","39","41","42"]
["","","","Silent operation","dBA","20","","","31","33","34"]
["","","","Low","dBA","26","","","34","36","37"]
["","","","High","dBA","40","","","43","45","46"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1"]
["","Infrared remote control","","","","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2"]
["","Remote control holder","","","","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2"]
["Control systems","Wired remote control","","","","BRC944B2, BRC073A1","","","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","","","ARC470A1","ARC470A1","ARC470A1"]
["Piping connections","Liquid","","OD","mm","6.35","","","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.50","","","12.7","12.7","12.7"]
["","Drain","","","","18","","","18","18","18"]
["Power input","Cooling","","Nom.","kW","0.019","","","0.029","0.032","0.032"]
["","Heating","","Nom.","kW","0.020","","","0.032","0.035","0.035"]
["Sound power level","Cooling","","","dBA","55","","","59","60","62"]
["","Heating","","","dBA","55","","","61","62","62"]
["Dimensions","Unit","","Width","mm","770","","","990","990","990"]
["","","","Depth","mm","225","","","263","263","263"]
["","","","Height","mm","286","","","295","295","295"]
["Casing","Colour","","","","White","","","White","White","White"]
["Weight","Unit","","","kg","8.50","","","13.5","13.5","13.5"]
["Fan","Air flow rate","Heating","High","m³/min","10.3","","","17.3","17.9","17.9"]
["","","","Medium","m³/min","8.6","","","14.8","15.8","15.8"]
["","","","Low","m³/min","6.7","","","12.2","12.8","12.8"]
["","","","Silent operation","m³/min","5.3","","","10.7","11.3","11.3"]
["","","Cooling","Low","m³/min","6.1","","","11.9","12.2","12.2"]
["","","","Medium","m³/min","8.1","","","14.4","14.8","14.8"]
["","","","High","m³/min","10.1","","","16.8","17.3","17.3"]
["","","","Silent operation","m³/min","4.4","","","10.5","10.7","10.7"]
["Power supply","Phase","","","","1~","","","1~","1~","1~"]
["","Name","","","","","","","V1","V1","V1"]
["","Frequency","","","Hz","50","","","50","50","50"]
["","Voltage","","","V","220-240","","","220-240","220-240","220-240"]
["Power input","Cooling","","Nom.","kW","","0.019","0.032"]
["","Heating","","Nom.","kW","","0.02","0.032"]
["Casing","Colour","","","","","White","White"]
["Dimensions","Unit","","Height","mm","","286","286"]
["","","","Width","mm","","770","770"]
["","","","Depth","mm","","225","225"]
["Weight","Unit","","","kg","","8.5","9"]
["Fan","Air flow rate","Cooling","High","m³/min","","10.1","11.5"]
["","","","Medium","m³/min","","8.1","8.3"]
["","","","Low","m³/min","","6.1","6.3"]
["","","","Silent operation","m³/min","","4.4","4.5"]
["","","Heating","High","m³/min","","10.3","11.5"]
["","","","Medium","m³/min","","8.6","9"]
["","","","Low","m³/min","","6.7","7"]
["","","","Silent operation","m³/min","","5.3","5.3"]
["Sound power level","Cooling","","","dBA","","55","58"]
["","Heating","","","dBA","","55","58"]
["Sound pressure level","Cooling","","High","dBA","","40","43"]
["","","","Medium","dBA","","33","34"]
["","","","Low","dBA","","26","27"]
["","","","Silent operation","dBA","","20","20"]
["","Heating","","High","dBA","","40","40"]
["","","","Medium","dBA","","34","35"]
["","","","Low","dBA","","28","29"]
["","","","Silent operation","dBA","","21","21"]
["Piping connections","Liquid","","OD","mm","","6.35","6.35"]
["","Gas","","OD","mm","","9.5","9.5"]
["","Drain","","","","","18","18"]
["Control systems","Infrared remote control","","","","","ARC470A1","ARC470A1"]
["","Wired remote control","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Power supply","Phase","","","","","1~","1~"]
["","Frequency","","","Hz","","50","50"]
["","Voltage","","","V","","220-240","220-240"]