{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":9,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-C"]
[]
[]
[]
[]
["","","","","","ATXF20C5V1B","ATXF25C5V1B","ATXF35C5V1B","ATXF42C5V1B"]
["Sound pressure level","Heating","","High","dBA","39.0","40.0","","44.0"]
["","","","Medium","dBA","34.0","34.0","","34.0"]
["","","","Silent operation","dBA","21.0","21.0","","22.0"]
["","","","Low","dBA","28.0","28.0","","28.0"]
["","Cooling","","Medium","dBA","33.0","33.0","","36.0"]
["","","","Silent operation","dBA","20.0","20.0","","22.0"]
["","","","Low","dBA","25.0","26.0","","30.0"]
["","","","High","dBA","39.0","40.0","","45.0"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Batteries","","","","1","1","1","1"]
["","Infrared remote control","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","Remote control holder","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["Control systems","Wired remote control","","","","BRC073A1","BRC073A1","","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","","ARC470A1"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","","6.35"]
["","Gas","","OD","mm","9.50","9.50","","9.50"]
["","Drain","","","","18","18","","18"]
["Power input","Cooling","","Nom.","kW","0.023","0.023","","0.040"]
["","Heating","","Nom.","kW","0.023","0.023","","0.040"]
["Sound power level","Cooling","","","dBA","53.0","54.0","","59.0"]
["","Heating","","","dBA","55.0","55.0","","59.0"]
["Dimensions","Unit","","Width","mm","770","770","","770"]
["","","","Depth","mm","225","225","","225"]
["","","","Height","mm","286","286","","286"]
["Casing","Colour","","","","White","White","","White"]
["Weight","Unit","","","kg","8.00","8.00","","9.00"]
["Power supply","Phase","","","","1~","1~","","1~"]
["","Frequency","","","Hz","50","50","","50"]
["","Voltage","","","V","220-440","220-440","","220-440"]
["Power input","Cooling","","Nom.","kW","","","0.029"]
["","Heating","","Nom.","kW","","","0.029"]
["Casing","Colour","","","","","","White"]
["Dimensions","Unit","","Height","mm","","","286"]
["","","","Width","mm","","","770"]
["","","","Depth","mm","","","225"]
["Weight","Unit","","","kg","","","8.5"]
["Fan","Air flow rate","Cooling","High","m³/min","","","11.8"]
["","","","Medium","m³/min","","","8"]
["","","","Low","m³/min","","","6.4"]
["","","","Silent operation","m³/min","","","4.4"]
["","","Heating","High","m³/min","","","11.9"]
["","","","Medium","m³/min","","","8.6"]
["","","","Low","m³/min","","","6.5"]
["","","","Silent operation","m³/min","","","5.3"]
["Sound power level","Cooling","","","dBA","","","54"]
["","Heating","","","dBA","","","56"]
["Sound pressure level","Cooling","","High","dBA","","","43"]
["","","","Medium","dBA","","","34"]
["","","","Low","dBA","","","27"]
["","","","Silent operation","dBA","","","20"]
["","Heating","","High","dBA","","","40"]
["","","","Medium","dBA","","","35"]
["","","","Low","dBA","","","29"]
["","","","Silent operation","dBA","","","21"]
["Piping connections","Liquid","","OD","mm","","","6.35"]
["","Gas","","OD","mm","","","9.5"]
["","Drain","","","","","","18"]
["Control systems","Infrared remote control","","","","","","ARC470A1"]
["","Wired remote control","","","","","","BRC073A1"]
["Power supply","Phase","","","","","","1~"]
["","Frequency","","","Hz","","","50"]
["","Voltage","","","V","","","220-440"]