{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":7,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-M / ARXM-M"]
[]
[]
[]
[]
["","","","","ATXM25M2V1B / ARXM25M2V1B","ATXM35M2V1B / ARXM35M2V1B","ATXM50M2V1B / ARXM50MV1B"]
["Cooling capacity","Min.","","kW","1.3","1.4","1.7"]
["","Max.","","kW","3.2","4.0","5.3"]
["","Nom.","","kW","2.5","3.40","5.02"]
["Space cooling","SEER","","","8.50","8.50","7.31"]
["","Annual energy consumption","","kWh/a","103","140","239"]
["","Capacity","Pdesign","kW","2.50","3.40","5.00"]
["","Energy efficiency class","","","A+++","A+++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.40","2.50","4.60"]
["","SCOP/A","","","5.10","5.10","4.60"]
["","Energy efficiency class","","","A+++","A+++","A++"]
["","Annual energy consumption","","kWh/a","659","686","1,400"]
["Nominal efficiency","Annual energy consumption","","kWh","285","416","728"]
["","EER","","","4.39","4.09","3.45"]
["","COP","","","5.00","4.04","3.79"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","A","A","A"]
["Heating capacity","Nom.","","kW","2.8","4.00","5.8"]
["","Min.","","kW","1.3","1.4","1.7"]
["","Max.","","kW","4.7","5.2","6.5"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]