{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":15,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-L / 2AMXM-M9"]
[]
[]
[]
[]
["","","","","ATXP20L2V1B / ATXP20L2V1B / 2AMXM40M4V1B9","ATXP20L2V1B / ATXP25L2V1B / 2AMXM40M4V1B9","ATXP20L2V1B / ATXP35L2V1B / 2AMXM40M4V1B9","ATXP25L2V1B / ATXP25L2V1B / 2AMXM40M4V1B9","ATXP25L2V1B / ATXP35L2V1B / 2AMXM40M4V1B9","ATXP20L2V1B / ATXP20L2V1B / 2AMXM50M4V1B9","ATXP20L2V1B / ATXP25L2V1B / 2AMXM50M4V1B9","ATXP20L2V1B / ATXP35L2V1B / 2AMXM50M4V1B9","ATXP25L2V1B / ATXP25L2V1B / 2AMXM50M4V1B9","ATXP25L2V1B / ATXP35L2V1B / 2AMXM50M4V1B9","ATXP35L2V1B / ATXP35L2V1B / 2AMXM50M4V1B9"]
["Cooling capacity","Nom.","","kW","4.00","4.00","4.00","4.00","4.00","4.00","4.50","5.00","5.00","5.00","5.00"]
["Space cooling","SEER","","","7.28","7.28","6.99","7.14","6.93","7.43","7.47","7.34","7.32","7.29","7.20"]
["","Annual energy consumption","","kWh/a","193","193","201","196","202","189","211","239","239","240","243"]
["","Capacity","Pdesign","kW","4.00","4.00","4.00","4.00","4.00","4.00","4.50","5.00","5.00","5.00","5.00"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","3.20","3.20","3.20","3.20","3.20","4.00","4.10","4.20","4.20","4.20","4.20"]
["","SCOP/A","","","4.15","4.10","4.05","4.01","3.96","4.14","4.16","4.18","4.17","4.19","4.22"]
["","Energy efficiency class","","","A+","A+","A+","A+","A","A+","A+","A+","A+","A+","A+"]
["","Annual energy consumption","","kWh/a","1,078","1,092","1,104","1,116","1,130","1,350","1,378","1,406","1,408","1,404","1,393"]
["Nominal efficiency","Annual energy consumption","","kWh","583","570","573","575","567","556","630","731","735","742","740"]
["","EER","","","3.43","3.51","3.49","3.48","3.53","3.60","3.57","3.42","3.40","3.37","3.38"]
["","COP","","","3.97","4.01","4.09","4.06","4.14","3.61","3.63","3.65","3.61","3.61","3.63"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","4.20","4.20","4.20","4.20","4.20","5.20","5.60","5.60","5.60","5.60","5.60"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]