{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":5,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-M"]
[]
[]
[]
[]
["","","","","CTXM15M2V1B"]
["Sound pressure level","Heating","High","dBA","39"]
["","","Silent operation","dBA","20"]
["","","Low","dBA","26"]
["","Cooling","Silent operation","dBA","19"]
["","","Low","dBA","25"]
["","","High","dBA","41"]
["","","Nom.","dBA","34"]
["","Cooling","Nom.","dBA","33"]
["Standard Accessories","Installation manual","","","1"]
["","Operation manual","","","1"]
["","Infrared remote control","","","1"]
["","AAA dry-cell batteries","","","2"]
["","Remote control holder","","","1"]
["","Mounting plate","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","1"]
["","Indoor unit fixing screws","","","2"]
["Control systems","Wired remote control","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC466A33"]
["Piping connections","Liquid","OD","mm","6.35"]
["","Gas","OD","mm","9.5"]
["","Drain","","","18"]
["Sound power level","Cooling","","dBA","57"]
["","Heating","","dBA","54"]
["Dimensions","Unit","Width","mm","811"]
["","","Depth","mm","272"]
["","","Height","mm","294"]
["Casing","Colour","","","White"]
["Weight","Unit","","kg","10"]
["Power supply","Phase","","","1~"]
["","Name","","","V1"]
["","Frequency","","Hz","50"]
["","Voltage","","V","220-240"]
["Notes","","","","(1) - SL: The silent fan level of the air flow rate setting"]