{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":7,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B","CTXM15R5V1B"]
["Power input","Cooling","","Nom.","kW","0.029","0.029"]
["","Heating","","Nom.","kW","0.023","0.023"]
["Casing","Colour","","","","White","White"]
["Dimensions","Unit","","Height","mm","295","295"]
["","","","Width","mm","778","778"]
["","","","Depth","mm","272","272"]
["Weight","Unit","","","kg","10","10"]
["Fan","Air flow rate","Cooling","High","m³/min","10.5","10.5"]
["","","","Medium","m³/min","7.5","7.5"]
["","","","Low","m³/min","5.7","5.7"]
["","","","Silent operation","m³/min","4.3","4.3"]
["","","Heating","High","m³/min","9.3","9.3"]
["","","","Medium","m³/min","8.2","8.2"]
["","","","Low","m³/min","6.2","6.2"]
["","","","Silent operation","m³/min","5.1","5.1"]
["Sound power level","Cooling","","","dBA","57","57"]
["","Heating","","","dBA","54","54"]
["Sound pressure level","Cooling","","High","dBA","41","41"]
["","","","Medium","dBA","33","33"]
["","","","Low","dBA","25","25"]
["","","","Silent operation","dBA","19","19"]
["","Heating","","High","dBA","39","39"]
["","","","Medium","dBA","34","34"]
["","","","Low","dBA","26","26"]
["","","","Silent operation","dBA","20","20"]
["Piping connections","Liquid","","OD","mm","6.35","6.35"]
["","Gas","","OD","mm","9.5","9.5"]
["","Drain","","","","18","18"]
["Control systems","Infrared remote control","","","","ARC466A67","ARC466A67"]
["","Wired remote control","","","","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","WLAN adapter kit","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Energy Efficiency Range","","","","","A+++ ~ D","A+++ ~ D"]
["Power supply","Name","","","","V1","V1"]
["","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]