{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":11,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2CND-A4A"]
[]
[]
[]
[]
["","","","","","D2CND024A4AB","D2CND024A4AA","D2CND028A4AB","D2CND028A4AA","D2CND035A4AA","D2CND035A4AB"]
["Gas","Consumption (G20)","","Min","m³/h","0.31","0.31","0.511","0.511","0.511","0.511"]
["","","","Max","m³/h","2.48","2.48","2.89","2.89","3.63","3.63"]
["","Consumption (G25)","","Min","m³/h","0.36","0.36","0.59","0.59","0.59","0.59"]
["","","","Max","m³/h","2.89","2.89","3.32","3.32","4.19","4.19"]
["","Consumption (G31)","","Min","m³/h","0.12","0.12","0.2","0.2","0.2","0.2"]
["","","","Max","m³/h","0.96","0.96","1.1","1.1","1.38","1.38"]
["","NOx class","","","","6","6","6","6","6","6"]
["","NOx level (G20)","","","mg/kWh","22","22","36.3","36.3","35.5","35.5"]
["Central heating","Heat input Qn (net calorific value)","Nom","Min","kW","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Max","kW","23.5","23.5","27","27","34","34"]
["","Heat input Qn (gross calorific value)","Nom","Min","kW","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Max","kW","26.1","26.1","30","30","37.8","37.8"]
["","Output Pn at 80/60°C","","Min","kW","2.8","2.8","4.6","4.6","4.6","4.6"]
["","","","Nom","kW","22.8","22.8","26.3","26.3","33.2","33.2"]
["","Output Pnc at 50/30°C","","Min","kW","3.1","3.1","5.2","5.2","5.2","5.2"]
["","","","Nom","kW","24","24.0","28.2","28.2","35","35"]
["","Output at 37/30°C","","Nom","kW","7.6","7.6","8.8","8.8","11.1","11.1"]
["","Water temperature","","Max","°C","100","100","100","100","100","100"]
["","Efficiency","","Net calorific value","%","97.9","97.9"]
["","","","Gross calorific value","%","87.3","87.3"]
["Domestic hot water","Heat input (net calorific value) Qnw","Nom","Min","kW","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Max","kW","23.5","23.5","29.5","29.5","34","34"]
["","Heat input (gross calorific value) Qnw","Nom","Min","kW","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Max","kW","26.1","26.1","32.7","32.7","37.7","37.7"]
["","Temperature","","Max","°C","60","60","60","60","60","60"]
["Heat losses","Stand-by boiler Ps","","","kW","0.057","0.057","0.065","0.0650","0.0650","0.065"]
["Supply air","Connection","","","mm","100","100","100","100","100","100"]
["","Concentric","","","","Yes","Yes","Yes","Yes","Yes","Yes"]
["Flue gas","Temperature","","Max","°C","90","90","76.4","76.4","81.7","81.7"]
["","Connection","","","mm","60","60","60","60","60","60"]
["","Mass flow (G20)","","Max","kg/h","38.7","38.7","55.7","44.5","55.7","55.7"]
["","Mass flow (G31)","","Max","kg/h","36","36.0","43.3","43.3","54.7","54.7"]
["Casing","Colour","","","","Titanium White (Ral9003)","Titanium White (Ral9003)","Titanium White (Ral9003)","Titanium White (Ral9003)","Titanium White (Ral9003)","Titanium White (Ral9003)"]
["","Material","","","","Sheet metal","Sheet metal","Powder painted galvanised steel plate","Powder painted galvanised steel plate","Powder painted galvanised steel plate","Powder painted galvanised steel plate"]
["Dimensions","Unit","Height","Casing","mm","590","590","690","690","690","690"]
["","","","Width","mm","400","400","440","440","440","440"]
["","","","Depth","mm","256","256","295","295","295","295"]
["Weight","Unit","","Empty","kg","27","27","37","37","37","37"]
["","","","Full","kg","27","27","","39","39"]
["","Boiler","","Empty","kg","27","27.0"]
["Domestic hot water heating","General","","Declared load profile","","XL","XL","XL","XL","XL","XL"]
["","","","Water heating energy efficiency class","","A","A","A","A","A","A"]
["Space heating","General","","Seasonal space heating eff. class","","A","A","A","A","A","A"]
["Flue gas","Mass flow (G25)","","Max","kg/h","","","39.3","39.3","49.6","49.6"]