{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":8,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2CND-A5A"]
[]
[]
[]
[]
["","","","","","D2C18ND024A5AA","D2C20ND028A5AA","D2C24ND035A5AA"]
["Gas","Consumption (G20)","","Min","m³/h","0.31","0.51","0.51"]
["","","","Max","m³/h","1.80","2.04","2.45"]
["","Consumption (G25)","","Min","m³/h","0.36","0.59","0.59"]
["","","","Max","m³/h","2.09","2.35","2.85"]
["","Consumption (G31)","","Min","m³/h","0.12","0.20","0.20"]
["","","","Max","m³/h","0.69","0.98","1.19"]
["","NOx class","","","","6","6","6"]
["","NOx level (G20)","","","mg/kWh","18","31","32"]
["Central heating","Heat input Qn (net calorific value)","Nom","Min","kW","2.9","4.8","4.8"]
["","","","Max","kW","16.9","19.2","23.5"]
["","Heat input Qn (gross calorific value)","Nom","Min","kW","3.2","5.3","5.3"]
["","","","Max","kW","18.8","21.3","26.1"]
["","Output Pn at 80/60°C","","Min","kW","2.8","4.6","4.6"]
["","","","Nom","kW","16.4","18.8","22.9"]
["","Output Pnc at 50/30°C","","Min","kW","3.1","5.2","5.2"]
["","","","Nom","kW","18.0","20.0","24.0"]
["","Output at 37/30°C","","Nom","kW","5.5","6.3","7.7"]
["","Water temperature","","Max","°C","100","100","100"]
["Domestic hot water","Heat input (net calorific value) Qnw","Nom","Min","kW","2.9","4.8","4.8"]
["","","","Max","kW","25.3","29.5","34.0"]
["","Heat input (gross calorific value) Qnw","Nom","Min","kW","3.2","5.3","5.3"]
["","","","Max","kW","27.7","32.7","37.7"]
["","Comfort class (EN13203)","","","","***","***","***"]
["","Temperature","","Max","°C","70","70","70"]
["Supply air","Connection","","","mm","100","100","100"]
["","Concentric","","","","Yes","Yes","Yes"]
["Flue gas","Temperature","","Max","°C","77","76","82"]
["","Connection","","","mm","60","60","60"]
["","Mass flow (G20)","","Max","kg/h","38.7","44.5","55.7"]
["","Mass flow (G31)","","Max","kg/h","36.0","43.3","54.8"]
["Casing","Colour","","","","Titanium White (Ral9003)","Titanium White (Ral9003)","Titanium White (Ral9003)"]
["","Material","","","","Powder painted galvanised steel plate","Powder painted galvanised steel plate","Powder painted galvanised steel plate"]
["Dimensions","Unit","Height","Casing","mm","590","695","695"]
["","","","Width","mm","400","440","440"]
["","","","Depth","mm","256","295","295"]
["Weight","Unit","","Empty","kg","27","37","37"]
["Domestic hot water heating","General","","Declared load profile","","XL","XL","XL"]
["","","","Water heating energy efficiency class","","A","A","A"]
["Space heating","General","","Seasonal space heating eff. class","","A","A","A"]