{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":78,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DB-O"]
[]
[]
[]
[]
["","","","","","BDB710DB13XXA","BDB710DB13XXB","MDB106EA12XXA","MDB106EA12XXB","MDB107EA12XXA","MDB107EA12XXB","BDB110DA12XXA","BDB110DA12XXB","BDB112DA12XXA","BDB112DA12XXB","BDB117DA12XXA","BDB117DA12XXB","SB.BD121NO118D","SB.BD121TO118D","SB.MDB121TO118E","SB.BD123TO118D","SB.MDB123TO118E","BDB713DB13XXA","BDB713DB13XXB","SB.BD135NO50D","SB.BD135TO50D","SB.MDB135NO50E","SB.MDB135TO50E","SB.MDB140TO50E","MDB212EB12XXA","MDB212EB12XXB","BDB218DA12XXA","BDB218DA12XXB","BDB220DB12XXA","BDB220DB12XXB","SB.BD221NO118D","SB.BD221TO50D","SB.MDB221NO118E","SB.MDB221TO50E","PDB221TO02DA","PDB221TO02DB","SB.MDB235TO02E","MDB315EB13XXA","MDB315EB13XXB","BDB320DB13XXA","BDB320DB13XXB","MDB320EB13XXA","MDB320EB13XXB","BDB330DB13XXA","BDB330DB13XXB","PDB330DB11XXA","PDB330DB11XXB","SB.MDB335NO02E","SB.MDB335TO02E","SB.MDB340NO02E","SB.MDB340TO02E","MDB425EB13XXA","MDB425EB13XXB","BDB440DB13XXA","BDB440DB13XXB","BDB445DB13XXA","BDB445DB13XXB","MDB530EB13XXA","MDB530EB13XXB","BDB550DB13XXA","BDB550DB13XXB","MDB635EB13XXA","MDB635EB13XXB","MDB645EB13XXA","MDB645EB13XXB","BDB660DB13XXA","BDB660DB13XXB","BDB680DB13XXA","BDB680DB13XXB","MDB706EB13XXA","MDB706EB13XXB","MDB707EB13XXA","MDB707EB13XXB"]
["Refrigerant","GWP","","","","","","","","","","","","","","","","2,142","2,142","1,430.0","2,142","1,430","","","2,142","2,142","1,430","1,430","1,430","","","","","","","2,142","2,142","1,430","1,430","","","1,430","","","","","","","","","","","1,430","1,430","1,430","1,430"]
["","Type","","","","","","","","","","","","","","","","R-452A","R-452A","R-134a","R-452A","R-134a","","","R-452A","R-452A","R-134a","R-134a","R-134a","","","","","","","R-452A","R-452A","R-134a","R-134a","","","R-134a","","","","","","","","","","","R-134a","R-134a","R-134a","R-134a"]
["Refrigerating capacity","Medium temperature","R-134a","Nom","kW","","","","","","","","","","","","","","","1.140 (1)","","1.422 (1)","","","","","3.188 (1)","3.492 (1)","3.606 (1)","","","","","","","","","1.816 (1)","2.029 (1)","","","5.070 (1)","","","","","","","","","","","7.293 (1)","8.779 (1)","11.014 (1)","14.069 (1)"]
["","Low temperature","R-452A","Nom","kW","","","","","","","","","","","","","0.662 (1)","0.905 (1)","","1.088 (1)","","","","2.384 (1)","2.38 (1)","","","","","","","","","","1.342 (1)","1.719 (1)"]
["Standard liquid receiver","l","","","","15","","1.6","","2.5","","1.6","","1.6","","1.6","","1.6","1.6","1.6","1.6","2.5","15","","2.5","2.5","2.5","2.5","5.6","2.5","","2.5","","2.5","","2.5","2.5","2.5","2.5","2.5","","10","2.5","","2.5","","2.5","","2.5","","2.5","","15","15","15","15","5.6","","5.6","","5.6","","10","","10","","15","","15","","15","","15","","15","","15"]
["Operation range","Cold room temperature","","Min.","°C","","","","","","","","","","","","","-25","-25","-5","-25","-5","","","-25","-25","-5","-5","-5","","","","","","","-25","-25","-5","-5","","","-5","","","","","","","","","","","-5","-5","-5","-5"]
["","","","Max.","°C","","","","","","","","","","","","","-15","-15","10","-15","10","","","-15","-15","10","10","10","","","","","","","-15","-15","10","10","","","10","","","","","","","","","","","10","10","10","10"]
["Defrost","","","","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","Electric","Electric","Electric","Electric","Electric","","Electric","Electric","Electric","Electric","Electric","Electric","","Electric","","Electric","","Electric","Electric","Electric","Electric","Electric","","Electric","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","Electric","Electric","Electric","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric"]
["Dimensions","Evaporator unit","","Depth","mm","","","","","","","","","","","","","410","410","410","410","410","","","410","410","410","410","690","","","","","","","410","410","410","410","","","690","","","","","","","","","","","690","690","700","700"]
["","","","Height","mm","","","","","","","","","","","","","215","215","215","215","215","","","215","215","215","215","545","","","","","","","215","215","215","215","","","530","","","","","","","","","","","600","600","620","620"]
["","","","Width","mm","","","","","","","","","","","","","614","614","614","614","614","","","1,614","1,614","1,614","1,614","805","","","","","","","1,034","1,034","1,034","1,034","","","1,220","","","","","","","","","","","1,690","1,690","1,840","1,840"]
["","Condensing unit","","Depth","mm","","","","","","","","","","","","","337","337","337","337","337","","","427","427","427","427","540","","","","","","","427","427","427","427","","","532","","","","","","","","","","","642","642","742","742"]
["","","","Width","mm","","","","","","","","","","","","","620","620","620","620","620","","","820","820","820","820","920","","","","","","","820","820","820","820","","","1,075","","","","","","","","","","","1,575","1,575","1,725","1,725"]
["Compressor","Nominal power","","","kW","","","","","","","","","","","","","0.75","1.1","0.4","1.3","0.7","","","2.2","2.2","2.2","2.6","2.94","","","","","","","1.3","1.5","0.9","1.7","","","3.7","","","","","","","","","","","4.8","6.3","7.4","9.555"]
["","Type","","","","","","","","","","","","","","","","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","","","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","","","","","","","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","","","Hermetic Reciprocating","","","","","","","","","","","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating","Hermetic Reciprocating"]
["","Starting method","","","","","","","","","","","","","","","","Direct","Direct","Direct","Direct","Direct","","","","Direct","Direct","Direct","Direct","","","","","","","Direct","Direct","Direct","Direct","","","Direct","","","","","","","","","","","Direct","Direct","Direct","Direct"]
["Condenser","Air flow","","","m³/h","","","","","","","","","","","","","750","750","750","750","750","","","1,500","1,500","1,500","1,500","3,150","","","","","","","1,400","1,400","1,400","1,400","","","3,200","","","","","","","","","","","5,500","7,000","8,100","8,100"]
["Evaporator","Air flow","","","m³/h","","","","","","","","","","","","","600","600","600","600","600","","","1,800","1,800","1,800","1,800","2,300","","","","","","","1,200","1,200","1,200","1,200","","","4,600","","","","","","","","","","","6,800","6,400","8,400","8,000"]
["","Air throw","","","m","","","","","","","","","","","","","4 (2)","4 (2)","4 (2)","4 (2)","4 (2)","","","4 (2)","4 (2)","4 (2)","4 (2)","12 (2)","","","","","","","4 (2)","4 (2)","4 (2)","4 (2)","","","11 (2)","","","","","","","","","","","11 (2)","11 (2)","13 (2)","12 (2)"]
["Defrost heaters","W","","","","6400","","450","","450","","450","","450","","450","","450","450","450","450","450","6400","","1,400","1,400","1,400","1,400","1,400","800","","800","","800","","800","800","800","800","800","","3,000","1400","","1400","","1400","","1400","","1400","","4,000","4,000","4,800","4,800","1400","","1400","","1400","","3150","","3250","","4900","","4900","","5000","","5000","","6300","","6300"]
["Power supply","Phase","","","","","","","","","","","","","","","","1~","1~","1~","1~","1~","","","3N~","3N~","3N~","3N~","3N~","","","","","","","1~","3N~","1~","3N~","","","3N~","","","","","","","","","","","3N~","3N~","3N~","3N~"]
["","Frequency","","","Hz","","","","","","","","","","","","","50","50","50","50","50","","","50","50","50","50","50","","","","","","","50","50","50","50","","","50","","","","","","","","","","","50","50","50","50"]
["","Voltage","","","V","","","","","","","","","","","","","230","230","230","230","230","","","400","400","400","400","400","","","","","","","230","400","230","400","","","400","","","","","","","","","","","400","400","400","400"]
["Notes","","","","","","","","","","","","","","","","","(1) - When normally running: -20°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: 0°C / +30°C","","","(1) - When normally running: -20°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","","","","","","","(1) - When normally running: -20°C / +30°C","(1) - When normally running: -20°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","","","(1) - When normally running: 0°C / +30°C","","","","","","","","","","","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C","(1) - When normally running: 0°C / +30°C"]
["","","","","","","","","","","","","","","","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","","","","","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","","","","","","","","","","","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc.","(2) - Use air throw as a base.  Air throw is affected by many factors such as height of room, product storage, location of evaporator, etc."]
["","","","","","","","","","","","","","","","","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","","","","","","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","","","(3) - Contains fluorinated greenhouse gases","","","","","","","","","","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases"]
["Refrigerating capacity","Low temperature","R-452A","Nom","kW","11.537","","","","","","0.662","","0.905","","1.164","","","","","","","12.735","","","","","","","","","1.436","","1.719","","","","","","","","","","","2.384","","","","2.581","","","","","","","","","","3.283","","3.604","","","","4.925","","","","","","7.492","","8.94"]
["Casing","Colour","","Condensing unit","","White","White","White","White","White","White","White","White","White","White","White","White","","","","","","White","White","","","","","","White","White","White","White","White","White","","","","","White","White","","White","White","White","White","White","White","White","White","White","White","","","","","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White","White"]
["Dimensions","Condensing unit","","Width","mm","1725","","682","","682","","682","","682","","682","","","","","","","1725","","","","","","","882","","882","","882","","","","","","882","","","882","","882","","882","","882","","882","","","","","","920","","920","","920","","1075","","1075","","1575","","1575","","1575","","1575","","1725","","1725"]
["","","","Depth","mm","770","","337","","337","","337","","337","","337","","","","","","","770","","","","","","","427","","427","","427","","","","","","427","","","427","","427","","427","","427","","427","","","","","","540","","540","","540","","560","","560","","670","","670","","670","","670","","770","","770"]
["Compressor","Quantity","","","","1","","1","","1","","1","","1","","1","","","","","","","1","","","","","","","1","","1","","1","","","","","","1","","","1","","1","","1","","1","","1","","","","","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1","","1"]
["","Type","","","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","","","","","","Hermetic","","","","","","","Hermetic","","Hermetic","","Hermetic","","","","","","Hermetic","","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","","","","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic","","Hermetic"]
["","Model","","","","S 10-52Y","","NJ6220Z","","NTU6222ZV","","NEU2178GK","","NJ2192GK","","NJ2212GK","","","","","","","S 15-56Y","","","","","","","TFH4518Y/T","","NJ2212GK","","TFH2480Z/T","","","","","","TFH2480Z/T","","","TFH4525Y/T","","TFH2511Z/T","","MTZ40JH4VE","","NTZ068A4","","NTZ068A4","","","","","","MTZ50HK4CVE","","NTZ096A4LR1B","","NTZ108A4LR1B","","MTZ64HM4","","NTZ 136A4LR1B","","MTZ80HP4","","MTZ100HS4","","NTZ215A4LR1B","","NTZ271A4 LR1B","","MTZ125HU4","","MTZ160HW4VE"]
["","Starting method","","","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","","","","","","Direct","","","","","","","Direct","","Direct","","Direct","","","","","","Direct","","","Direct","","Direct","","Direct","","Direct","","Direct","","","","","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct"]
["Condenser","Air flow","","","m³/h","8100","","750","","750","","750","","750","","750","","","","","","","8100","","","","","","","1400","","1400","","1400","","","","","","1400","","","1500","","1500","","1500","","1500","","1500","","","","","","3150","","3150","","3150","","3200","","3200","","5500","","7000","","7000","","7000","","8100","","8100"]
["Operation range","Cold room temperature","","Min.","°C","-25","","-5","","-5","","-25","","-25","","-25","","","","","","","-25","","","","","","","-5","","-25","","-25","","","","","","-5","","","-5","","-25","","-5","","-25","","-5","","","","","","-5","","-25","","-25","","-5","","-25","","-5","","-5","","-25","","-25","","-5","","-5"]
["","","","Max.","°C","-15","","10","","10","","-15","","-15","","-15","","","","","","","-15","","","","","","","10","","-15","","-15","","","","","","10","","","10","","-15","","10","","-15","","10","","","","","","10","","-15","","-15","","10","","-15","","10","","10","","-15","","-15","","10","","10"]
["","Ambient temperature","","Min.","°C","20","","20","","20","","20","","20","","20","","","","","","","20","","","","","","","20","","20","","20","","","","","","20","","","20","","20","","20","","20","","20","","","","","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20","","20"]
["","","","Max.","°C","45","","45","","45","","45","","45","","45","","","","","","","45","","","","","","","45","","45","","45","","","","","","45","","","45","","45","","45","","45","","45","","","","","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45","","45"]
["Refrigerant","Type","","","","R-452A","","R-134a","","R-134a","","R-452A","","R-452A","","R-452A","","","","","","","R-452A","","","","","","","R-134a","","R-452A","","R-452A","","","","","","R-452A","","","R-134a","","R-452A","","R-134a","","R-452A","","R-452A","","","","","","R-134a","","R-452A","","R-452A","","R-134a","","R-452A","","R-134a","","R-134a","","R-452A","","R-452A","","R-134a","","R-134a"]
["","GWP","","","","2140","","1430","","1430","","2140","","2140","","2140","","","","","","","2140","","","","","","","1430","","2140","","2140","","","","","","2140","","","1430","","2140","","1430","","2140","","2140","","","","","","1430","","2140","","2140","","1430","","2140","","1430","","1430","","2140","","2140","","1430","","1430"]
["Power supply","Voltage","","","V","380-400","","220-230","","220-230","","220-230","","220-230","","220-230","","","","","","","380-400","","","","","","","380-400","","220-230","","380-400","","","","","","380-400","","","380-400","","380-400","","380-400","","380-400","","380-400","","","","","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400","","380-400"]
["","Phase","","","","3N~","","1~","","1~","","1~","","1~","","1~","","","","","","","3N~","","","","","","","3N~","","1~","","3N~","","","","","","3N~","","","3N~","","3N~","","3N~","","3N~","","3N~","","","","","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~","","3N~"]
["","Frequency","","","Hz","50","","50","","50","","50","","50","","50","","","","","","","50","","","","","","","50","","50","","50","","","","","","50","","","50","","50","","50","","50","","50","","","","","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50","","50"]
["Dimensions","Evaporator unit","","Height","mm","","544","","215","","215","","215","","215","","215","","","","","","","544","","","","","","","215","","215","","215","","","","","","215","","","215","","215","","215","","215","","215","","","","","","545","","545","","545","","544","","544","","544","","544","","544","","544","","544","","544"]
["","","","Width","mm","","1975","","676","","676","","676","","676","","676","","","","","","","1975","","","","","","","1074","","1074","","1074","","","","","","1074","","","1676","","1676","","1676","","1676","","1676","","","","","","845","","845","","845","","1425","","1425","","1975","","1975","","1975","","1975","","1975","","1975"]
["","","","Depth","mm","","608","","410","","410","","410","","410","","410","","","","","","","608","","","","","","","410","","410","","410","","","","","","410","","","410","","410","","410","","410","","410","","","","","","690","","690","","690","","608","","608","","608","","608","","608","","608","","608","","608"]
["Evaporator","Air throw","","","m","","18","","4","","4","","4","","4","","4","","","","","","","18","","","","","","","4","","4","","4","","","","","","4","","","4","","4","","4","","4","","4","","","","","","12","","12","","12","","17","","17","","20","","20","","20","","20","","18","","18"]
["Refrigerating capacity","Medium temperature","R-134a","Nom","kW","","","1.14","","1.422","","","","","","","","","","","","","","","","","","","","1.816","","","","","","","","","","","","","3.188","","","","3.492","","","","","","","","","","3.948","","","","","","5.07","","","","7.293","","8.779","","","","","","11.014","","14.069"]