{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBBX-D6V / ERLA11-16DV3"]
[]
[]
[]
[]
["","","","","","EBBX16DF6V / ERLA16DAV3"]
["Heating capacity","Nom.","","","kW","16.0 (2) (1)"]
["Cooling capacity","Nom.","","","kW","13.8 (3), 15.9 (4)"]
["Power input","Heating","","Nom.","kW","3.53 (1), 4.56 (2)"]
["","Cooling","","Nom.","kW","4.68 (3), 3.82 (4)"]
["COP","","","","","4.53 (1), 3.51 (2)"]
["EER","","","","","2.94 (3), 4.16 (4)"]
["SEER","","","","","5.76 (5)"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.35"]
["","","","Seasonal space heating eff. class","","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.68"]
["","","","Seasonal space heating eff. class","","A+++"]
["Notes","","","","","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(3) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(4) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]
["","","","","","(5) - According to EN14825"]
["","","","","","(6) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(7) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["","","","","","(8) - Measured with a pressure drop of 10 kPa in the heating system at an operating condition of leaving water 47-55°C in a room with an ambient of 20°C. DB/WB 7°C/6°."]