{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBLQ-CV3"]
[]
[]
[]
[]
["","","","","","EBLQ05CAV3","EBLQ07CAV3"]
["Heating capacity","Nom.","","","kW","4.4, 4.03","7, 6.9"]
["Cooling capacity","Nom.","","","kW","3.88, 3.99","5.2, 5.15"]
["Power input","Cooling","","Nom.","kW","0.95, 1.93","1.37, 2.69"]
["","Heating","","Nom.","kW","0.88, 1.13","1.55, 2.45"]
["COP","","","","","5, 3.58","4.52, 3.42"]
["EER","","","","","4.07, 2.07","3.8, 2.1"]
["Dimensions","Unit","","Height","mm","735","735"]
["","","","Width","mm","1090","1090"]
["","","","Depth","mm","350","350"]
["Weight","Unit","","","kg","76","80"]
["Fan","Air flow rate","Heating","High","m³/min","45.0","47.0"]
["","","Cooling","High","m³/min","52.5","52.5"]
["Operation range","Heating","Water side","Min.","°C","15","15"]
["","","","Max.","°C","55.0","55.0"]
["","Cooling","Ambient","Min.","°CDB","10.0","10.0"]
["","","","Max.","°CDB","43.0","43.0"]
["","","Water side","Min.","°C","5.00","5.00"]
["","","","Max.","°C","22.0","22.0"]
["","Domestic hot water","Ambient","Min.","°CDB","-25.0","-25.0"]
["","","","Max.","°CDB","35.0","35.0"]
["","","Water side","Min.","°C","25","25"]
["","","","Max.","°C","80","80"]
["Sound power level","Heating","","Nom.","dBA","61","62"]
["","Cooling","","Nom.","dBA","63","63"]
["Sound pressure level","Heating","","Nom.","dBA","48","49"]
["","Cooling","","Nom.","dBA","48","50"]
["Refrigerant","Type","","","","R-410A","R-410A"]
["","GWP","","","","2088","2088"]
["","Charge","","","kg","1.3","1.45"]
["","Charge","","","tCO2Eq","2.714","3.027"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.22","3.22"]
["","","","Seasonal space heating eff. class","","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.45","4.18"]
["","","","Seasonal space heating eff. class","","A++","A++"]
["Power supply","Name","","","","V3","V3"]
["","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","230","230"]
["Notes","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["","","","","","(3) - Lower if back-up heater is installed; In case of no back-up heater, then heat pump operation starts at 10°C","(3) - Lower if back-up heater is installed; In case of no back-up heater, then heat pump operation starts at 10°C"]
["","","","","","(4) - For more details on standard accessories refer to Installation/operation manual","(4) - For more details on standard accessories refer to Installation/operation manual"]
["","","","","","(5) - Operation range domestic hot water (outdoor unit): range increase by support booster heater or backup heater. See separate drawing for operation range.","(5) - Operation range domestic hot water (outdoor unit): range increase by support booster heater or backup heater. See separate drawing for operation range."]
["","","","","","(6) -  > 50°C BSH only, no heatpump","(6) -  > 50°C BSH only, no heatpump"]
["","","","","","(7) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(7) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information."]
["","","","","","(8) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(8) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation)."]
["","","","","","(9) - Including piping + PHE; excluding expansion vessel","(9) - Including piping + PHE; excluding expansion vessel"]
["","","","","","(10) - Daikin Altherma inverter controlled compressor starting current always <= max. running current","(10) - Daikin Altherma inverter controlled compressor starting current always <= max. running current"]