{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSXB-D / ERLA11-16DV3"]
[]
[]
[]
[]
["","","","","","EBSXB16P30DF / ERLA16DAV3","EBSXB16P50DF / ERLA16DAV3"]
["Domestic hot water heating","General","","Declared load profile","","L","XL"]
["","Average climate","","Water heating energy efficiency class","","A+","A+"]
["COP","","","","","4.53 (1)","4.53 (1)"]
["Indoor unit","","","","","EBSXB16P30DF","EBSXB16P50DF"]
["Space heating","Average climate water outlet 35°C","General","ηs (Seasonal space heating efficiency)","%","184","184"]
["","","","Seasonal space heating eff. class","","A+++","A+++"]
["","","","SCOP","","4.68","4.68"]
["","Average climate water outlet 55°C","General","Seasonal space heating eff. class","","A++","A++"]
["","","","ηs (Seasonal space heating efficiency)","%","131","131"]
["","","","SCOP","","3.35","3.35"]
["Cooling capacity","Nom.","","","kW","13.6 (2)","13.6 (2)"]
["EER","","","","","2.91 (2)","2.91 (2)"]
["Heating capacity","Nom.","","","kW","16.0 (1)","16.0 (1)"]
["Power input","Heating","","Nom.","kW","3.53 (1)","3.53 (1)"]
["","Cooling","","Nom.","kW","4.68 (2)","4.68 (2)"]
["Notes","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]