{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Heating capacity","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Nom.","","","kW","10.3 (1), 9.2"]
["","Max.","","","kW","13, 11.9 (2)"]
["Power input","Nom.","","","kW","2.38 (1), 2.89 (2)"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Casing","Colour","","","","White"]
["","Material","","","","Precoated sheet metal"]
["Dimensions","Unit","","Height","mm","1730"]
["","","","Width","mm","600"]
["","","","Depth","mm","728"]
["Weight","Unit","","","kg","210"]
["Tank","Water volume","","","l","180"]
["","Insulation","","Heat loss","kWh/24h","1.36 (4)"]
["","Corrosion protection","","","","Anode"]
["Refrigerant","Type","","","","R-410A"]
["","GWP","","","","2090"]
["","Charge","","","tCO2Eq","3.76"]
["","Charge","","","kg","1.8"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.68"]
["","","","Seasonal space heating eff. class","","A++"]
["","Average climate water outlet 35°C","General","SCOP","","5.06"]
["","","","Seasonal space heating eff. class","","A+++"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Power supply","Name","","","","9W"]
["","Phase","","","","3~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","400"]
["Current","Recommended fuses","","","A","25"]
["Notes","","","","","(1) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)"]
["","","","","","(2) - EWB/LWB 0°C/-3°C - LWC 45°C (DT=5°C)"]
["","","","","","(3) - with 40% propylene glycol"]
["","","","","","(4) - Heatloss according to EN12897"]
["","","","","","(5) - Including piping + PHE + back-up heater; excluding expansion vessel"]
["","","","","","(6) - The sound pressure level is measured via a microphone at a 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment."]
["","","","","","(7) - By heat pump"]
["","","","","","(8) - By heat pump + back-up heater"]
["","","","","","(9) - By back-up heater"]