{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBX-E9W / ERGA04-08EV"]
[]
[]
[]
[]
["","","","","","EHBX08EF9W / ERGA06EAV3","EHBX08EA9W / ERGA06EAV3","EHBX08EA9W / ERGA08EAV3","EHBX08EF9W / ERGA08EAV3"]
["Heating capacity","Nom.","","","kW","6.00, 5.90","6.00 (1), 5.90 (2)","7.50, 7.80","7.50 (1), 7.80 (2)"]
["Cooling capacity","Nom.","","","kW","5.96, 5.09","5.96 (1), 5.09 (2)","6.25, 5.44","6.25 (1), 5.44 (2)"]
["Power input","Heating","","Nom.","kW","1.24, 1.69","1.24 (1), 1.69 (2)","1.63, 2.23","1.63 (1), 2.23 (2)"]
["","Cooling","","Nom.","kW","1.06, 1.55","1.06 (1), 1.55 (2)","1.16, 1.73","1.16 (1), 1.73 (2)"]
["COP","","","","","4.85, 3.50","4.85 (1), 3.50 (2)","4.60, 3.50","4.60 (1), 3.50 (2)"]
["EER","","","","","5.61, 3.28","5.61 (1), 3.28 (2)","5.40, 3.14","5.40 (1), 3.14 (2)"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.28","3.28","3.35","3.35"]
["","","","Seasonal space heating eff. class","","A++","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.52","4.52","4.61","4.61"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++"]
["Notes","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["Energy Efficiency Range","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]