{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":12,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSH-D / ERGA04-08DV"]
[]
[]
[]
[]
["","","","","","EHSH04P30DA / ERGA04DAV3","EHSH08P30DA / ERGA06DAV3","EHSH08P50DA / ERGA06DAV3","EHSH08P50DA7 / ERGA06DAV3","EHSH08P30DA / ERGA08DAV3","EHSH08P50DA / ERGA08DAV3","EHSH08P50DA7 / ERGA08DAV3"]
["Domestic hot water heating","General","","Declared load profile","","L","L","XL","","L","XL"]
["","Average climate","","Water heating energy efficiency class","","A","A","A","","A","A"]
["COP","","","","","5.10 (1), 3.65 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85, 3.50","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60, 3.50"]
["Indoor unit","","","","","EHSH04P30D","EHSH08P30D","EHSH08P50D","EHSH08P50DA7","EHSH08P30D","EHSH08P50D","EHSH08P50DA7"]
["Heating capacity","Nom.","","","kW","4.30 (1), 4.60 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Power input","Heating","","Nom.","kW","0.850 (1), 1.26 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["Notes","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["Heating capacity","Nom.","","","kW","","","","6.00, 5.90","","","7.50, 7.80"]
["Power input","Heating","","Nom.","kW","","","","1.24, 1.69","","","1.63, 2.23"]
["Domestic hot water heating","General","","Declared load profile","","","","","XL","","","XL"]
["","Average climate","","Water heating energy efficiency class","","","","","A","","","A"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","","","","3.26","","","3.32"]
["","","","Seasonal space heating eff. class","","","","","A++","","","A++"]
["","Average climate water outlet 35°C","General","SCOP","","","","","4.47","","","4.56"]
["","","","Seasonal space heating eff. class","","","","","A+++","","","A+++"]
["Energy Efficiency Range","","","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]