{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSHB-D3 / ERGA06-08EVH"]
[]
[]
[]
[]
["","","","","","EHSHB08P30DA3 / ERGA06EAV3H","EHSHB08P50DA3 / ERGA06EAV3H","EHSHB08P30DA3 / ERGA08EAV3H","EHSHB08P50DA3 / ERGA08EAV3H"]
["Domestic hot water heating","General","","Declared load profile","","L","XL","L","XL"]
["","Average climate","","Water heating energy efficiency class","","A+","A","A+","A"]
["COP","","","","","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["Indoor unit","","","","","EHSHB08P30DA3","EHSHB08P50DA3","EHSHB08P30DA3","EHSHB08P50DA3"]
["Space heating","Average climate water outlet 35°C","General","ηs (Seasonal space heating efficiency)","%","176","176","179","179"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++"]
["","","","SCOP","","4.47","4.47","4.56","4.56"]
["","Average climate water outlet 55°C","General","Seasonal space heating eff. class","","A++","A++","A++","A++"]
["","","","ηs (Seasonal space heating efficiency)","%","127","127","130","130"]
["","","","SCOP","","3.26","3.26","3.32","3.32"]
["Heating capacity","Nom.","","","kW","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Power input","Heating","","Nom.","kW","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["Notes","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]