{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":9,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-D3 / ERGA04-08EV"]
[]
[]
[]
[]
["","","","","","EHSX08P30DA3 / ERGA06EAV3","EHSX08P50DA3 / ERGA06EAV3","EHSX08P30DA3 / ERGA08EAV3","EHSX08P50DA3 / ERGA08EAV3"]
["Indoor unit","","","","","EHSX08P30DA3","EHSX08P50DA3","EHSX08P30DA3","EHSX08P50DA3"]
["Heating capacity","Nom.","","","kW","6.00, 5.90","6.00, 5.90","7.50, 7.80","7.50, 7.80"]
["Cooling capacity","Nom.","","","kW","5.96, 5.09","5.96, 5.09","6.25, 5.44","6.25, 5.44"]
["Power input","Heating","","Nom.","kW","1.24, 1.69","1.24, 1.69","1.63, 2.23","1.63, 2.23"]
["","Cooling","","Nom.","kW","1.06, 1.55","1.06, 1.55","1.16, 1.73","1.16, 1.73"]
["COP","","","","","4.85, 3.50","4.85, 3.50","4.60, 3.50","4.60, 3.50"]
["EER","","","","","5.61, 3.28","5.61, 3.28","5.40, 3.14","5.40, 3.14"]
["Domestic hot water heating","General","","Declared load profile","","L","XL","L","XL"]
["","Average climate","","Water heating energy efficiency class","","A+","A","A+","A"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.28","3.28","3.35","3.35"]
["","","","Seasonal space heating eff. class","","A++","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.52","4.52","4.61","4.61"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++"]
["Notes","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]