{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":11,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSXB-D"]
[]
[]
[]
[]
["","","","","","EHSXB04P30DA","EHSXB04P50DA7","EHSXB04P50DA","EHSXB08P30DA","EHSXB08P50DA7","EHSXB08P50DA"]
["Refrigerant","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0"]
["","Charge","","","kg","1.50","1.50","1.50","1.50","1.50","1.50"]
["","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["Operation range","Cooling","Ambient","Min.","°CDB","10","10","10","10","10","10"]
["","","Water side","Max.","°C","22","22","22","22","22","22"]
["","","","Min.","°C","5","5","5","5","5","5"]
["","Heating","Water side","Max.","°C","65","65","65","65","65","65"]
["","","","Min.","°C","18","18","18","18","18","18"]
["Sound power level","Nom.","","","dBA","39","39","39","39","39","39"]
["Dimensions","Unit","","Width","mm","595","790","790","595","790","790"]
["","","","Depth","mm","615","790","790","615","790","790"]
["","","","Height","mm","1,891","1,896","1,896","1,891","1,896","1,896"]
["Casing","Material","","","","Impact resistant polypropylene","Impact resistant polypropylene","Impact resistant polypropylene","Impact resistant polypropylene","Impact resistant polypropylene","Impact resistant polypropylene"]
["","Colour","","","","Traffic white (RAL9016) / Dark grey (RAL7011)","Traffic white (RAL9016) / Dark grey (RAL7011)","Traffic white (RAL9016) / Dark grey (RAL7011)","Traffic white (RAL9016) / Dark grey (RAL7011)","Traffic white (RAL9016) / Dark grey (RAL7011)","Traffic white (RAL9016) / Dark grey (RAL7011)"]
["Weight","Unit","","","kg","76.0","99.0","99.0","76.0","99.0","99.0"]
["PED","Category","","","","art. 3.3","art. 3.3","art. 3.3","art. 3.3","art. 3.3","art. 3.3"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","230","230","230","230","230","230"]
["Electric heater","Power supply","","Frequency","Hz","50","50","50","50","50","50"]
["","","","Name","","3V / 9W","3V / 9W","3V / 9W","3V / 9W","3V / 9W","3V / 9W"]
["","","","Phase","","1~ / 3~","1~ / 3~","1~ / 3~","1~ / 3~","1~ / 3~","1~ / 3~"]
["Notes","","","","","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","(5) - Heat up of tank only with heat pump, no electrical heater","(5) - Heat up of tank only with heat pump, no electrical heater","(5) - Heat up of tank only with heat pump, no electrical heater","(5) - Heat up of tank only with heat pump, no electrical heater","(5) - Heat up of tank only with heat pump, no electrical heater","(5) - Heat up of tank only with heat pump, no electrical heater"]