{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":27,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVH-D6V / ERGA04-08DV"]
[]
[]
[]
[]
["","","","","","EHVH04S23DA6V7 / ERGA04DAV3","EHVH08S18DA6V7 / ERGA06DAV3","EHVH08S18DA6V7 / ERGA08DAV3","EHVH08S23DA6V7 / ERGA06DAV3","EHVH08S23DA6V7 / ERGA08DAV3","EHVH04S18DA6V / ERGA04DAV3","EHVH04S18DJ6V / ERGA04DAV3","EHVH04S23DA6V / ERGA04DAV3","EHVH04S23DJ6V / ERGA04DAV3","EHVH04S18DA6V7 / ERGA04DAV3","EHVH04S18DJ6V7 / ERGA04DAV3","EHVH08S18DA6V / ERGA06DAV3","EHVH08S18DJ6V / ERGA06DAV3","EHVH08S23DA6V / ERGA06DAV3","EHVH08S23DJ6V / ERGA06DAV3","EHVH08S18DJ6V7 / ERGA06DAV3","EHVH08S23DJ6V7 / ERGA06DAV3","EHVH08S18DJ6V / ERGA08DAV3","EHVH08S23DA6V / ERGA08DAV3","EHVH08S23DJ6V / ERGA08DAV3","EHVH08S18DJ6V7 / ERGA08DAV3","EHVH08S23DJ6V7 / ERGA08DAV3"]
["Domestic hot water heating","General","","Declared load profile","","","","","","","L","L","XL","XL","","","L","L","XL","XL","","","L","XL","XL"]
["","Average climate","","Water heating energy efficiency class","","","","","","","A+","A+","A+","A+","","","A+","A+","A+","A+","","","A+","A+","A+"]
["COP","","","","","","","","","","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)","5.10, 3.65","5.10, 3.65","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85 (1), 3.50 (2)","4.85, 3.50","4.85, 3.50","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60, 3.50","4.60, 3.50"]
["Heat up time from 10°C to 50°C","hr","","","","","","","","","","","","","1h28min","1h28min","","","","","1h28min","1h40min","","","","1h28min","1h40min"]
["Heating capacity","Nom.","","","kW","","","","","","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)","","","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","","","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Power input","Heating","","Nom.","kW","","","","","","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)","","","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","","","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["Notes","","","","","","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Heating capacity","Nom.","","","kW","","","","","","","","","","4.30, 4.60","4.30, 4.60","","","","","6.00, 5.90","6.00, 5.90","","","","7.50, 7.80","7.50, 7.80"]
["Power input","Heating","","Nom.","kW","","","","","","","","","","0.850, 1.26","0.850, 1.26","","","","","1.24, 1.69","1.24, 1.69","","","","1.63, 2.23","1.63, 2.23"]
["","Domestic hot water from 10°C to 50°C","","Nom.","kWh","","","","","","","","","","2.48","2.48","","","","","2.48","3.01","","","","2.48","3.01"]
["Domestic hot water heating","General","","Declared load profile","","","","","","","","","","","L","L","","","","","L","XL","","","","L","XL"]
["","Average climate","","Water heating energy efficiency class","","","","","","","","","","","A+","A+","","","","","A+","A+","","","","A+","A+"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","","","","","","","","","","3.26","3.26","","","","","3.26","3.26","","","","3.32","3.32"]
["","","","Seasonal space heating eff. class","","","","","","","","","","","A++","A++","","","","","A++","A++","","","","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","","","","","","","","","","4.48","4.48","","","","","4.47","4.47","","","","4.56","4.56"]
["","","","Seasonal space heating eff. class","","","","","","","","","","","A+++","A+++","","","","","A+++","A+++","","","","A+++","A+++"]