{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVH-DVG / ERGA04-08DV"]
[]
[]
[]
[]
["","","","","","EHVH04S23DAVG / ERGA04DAV3","EHVH08S23DAVG / ERGA06DAV3","EHVH08S23DAVG / ERGA08DAV3"]
["Domestic hot water heating","General","","Declared load profile","","","XL","XL"]
["","Average climate","","Water heating energy efficiency class","","","A+","A+"]
["COP","","","","","5.10, 3.65","4.85 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["Heat up time from 10°C to 50°C","hr","","","","1h40min"]
["Heating capacity","Nom.","","","kW","","6.00 (1), 5.90 (2)","7.50 (1), 7.80 (2)"]
["Power input","Heating","","Nom.","kW","","1.24 (1), 1.69 (2)","1.63 (1), 2.23 (2)"]
["Notes","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["Heating capacity","Nom.","","","kW","4.30, 4.60"]
["Power input","Heating","","Nom.","kW","0.850, 1.26"]
["","Domestic hot water from 10°C to 50°C","","Nom.","kWh","3.01"]
["Domestic hot water heating","General","","Declared load profile","","XL"]
["","Average climate","","Water heating energy efficiency class","","A+"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.26"]
["","","","Seasonal space heating eff. class","","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.48"]
["","","","Seasonal space heating eff. class","","A+++"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]