{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":7,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHY2KOMB-A"]
[]
[]
[]
[]
["","","","","","EHY2KOMB28AA","EHY2KOMB32AA"]
["Domestic hot water","Heat input (gross calorific value) Qnw","Nom","Max","kW","32.3","36.3"]
["","","","Min","kW","7.9","8.4"]
["","Comfort class (EN13203)","","","","XL","XL"]
["","Temperature","","Max","°C","65","65"]
["","Heat input (net calorific value) Qnw","Nom","Min","kW","7.1","7.6"]
["","","","Max","kW","29.1","32.7"]
["Flue gas","Mass flow (G25)","","Max","kg/h","48.6","54.4"]
["","Mass flow (G20)","","Max","kg/h","48.6","54.4"]
["","Mass flow (G31)","","Max","kg/h","47.9","53.6"]
["","Temperature","","Max","°C","70","70"]
["Supply air","Concentric","","","","60/100","60/100"]
["Domestic hot water heating","General","","Water heating energy efficiency class","","A","A"]
["","","","Declared load profile","","XL","XL"]
["Dimensions","Unit","Height","Casing","mm","650","710"]
["Casing","Material","","","","Precoated sheet metal","Precoated sheet metal"]
["","Colour","","","","RAL9010","RAL9010"]
["Space heating","General","","ηs (Seasonal space heating efficiency)","%","92","93"]
["","","","Seasonal space heating eff. class","","A","A"]
["Central heating","Heat input Qn (gross calorific value)","Nom","Min","kW","7.9","8.4"]
["","","","Max","kW","26.3","30.0"]
["","Water temperature","","Max","°C","90","90"]
["","Output at 37/30°C","","Nom","kW","7.7","8.2"]
["","Output Pn at 80/60°C","","Min","kW","7.1","7.4"]
["","","","Nom","kW","23.1","26.6"]
["","Heat input Qn (net calorific value)","Nom","Min","kW","7.1","7.6"]
["","","","Max","kW","23.7","27.0"]
["","Output Pnc at 50/30°C","","Min","kW","7.7","8.2"]
["","","","Nom","kW","25.4","28.9"]
["Gas","NOx level (G20)","","","mg/kWh","27","36"]
["","Consumption (G25)","","Min","m³/h","0.84","0.89"]
["","","","Max","m³/h","3.46","3.92"]
["","NOx class","","","","6","6"]
["","Connection","","Diameter","mm","15","15"]
["","Consumption (G20)","","Max","m³/h","3.02","3.39"]
["","","","Min","m³/h","0.74","0.79"]
["","Consumption (G31)","","Min","m³/h","0.28","0.30"]
["","","","Max","m³/h","1.15","1.29"]