{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBH-AV3"]
[]
[]
[]
[]
["","","","","","EHYHBH05AAV3","EHYHBH08AAV3"]
["Casing","Colour","","","","White","White"]
["","Material","","","","Precoated sheet metal","Precoated sheet metal"]
["Dimensions","Unit","","Height","mm","902","902"]
["","","","Width","mm","450","450"]
["","","","Depth","mm","164","164"]
["Weight","Unit","","","kg","30.0","31.2"]
["PED","Category","","","","Art3§3, Excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","Category I"]
["Water side Heat exchanger","Water flow rate","Heating","Max.","l/min","23.0 (7)","23.5 (7)"]
["Sound power level","Nom.","","","dBA","42.0","42.0"]
["Operation range","Heating","Water side","Min.","°C","25 (8)","25 (8)"]
["","","","Max.","°C","55 (8)","55 (8)"]
["Power supply","Name","","","","V3","V3"]
["","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","230","230"]
["Wiring connections","For connection with user interface","","Quantity","","2","2"]
["","","","Remark","","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)"]
["Notes","","","","","(1) - Only for indoor unit","(1) - Only for indoor unit"]
["","","","","","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), boiler bypassed","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), boiler bypassed"]
["","","","","","(3) - DB/WB 7°C/6°C - LWC 45°C (DT=5°C), boiler bypassed","(3) - DB/WB 7°C/6°C - LWC 45°C (DT=5°C), boiler bypassed"]
["","","","","","(4) - Min. required","(4) - Min. required"]
["","","","","","(5) - Boiler bypassed","(5) - Boiler bypassed"]
["","","","","","(6) - For operation range of *HYHB* and *HYKOMB33AA, see operation range drawing","(6) - For operation range of *HYHB* and *HYKOMB33AA, see operation range drawing"]