{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHBRD-ADV1"]
[]
[]
[]
[]
["","","","","","EKHBRD011ADV1","EKHBRD014ADV1","EKHBRD016ADV1"]
["Sound pressure level","Nom.","","","dBA","43.0 (3), 46.0 (4), 0.00 (5), 0.00 (6)","45.0 (3), 46.0 (4), 0.00 (5), 0.00 (6)","46.0 (3), 46.0 (4), 0.00 (5), 0.00 (6)"]
["Refrigerant","Charge","","","TCO2Eq","3,718.000","3,718.000","3,718.000"]
["","GWP","","","","1,430","1,430","1,430"]
["","Charge","","","kg","2.60","2.60","2.60"]
["","Type","","","","R-134a","R-134a","R-134a"]
["Operation range","Heating","Water side","Max.","°C","80.0","80.0","80.0"]
["","","","Min.","°C","25","25","25"]
["Dimensions","Unit","","Width","mm","600","600","600"]
["","","","Depth","mm","695","695","695"]
["","","","Height","mm","705","705","705"]
["Casing","Material","","","","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal"]
["","Colour","","","","Metallic grey","Metallic grey","Metallic grey"]
["Weight","Unit","","","kg","144","144","144"]
["PED","Category","","","","Excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","Excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","Excluded from scope of PED due to article 1, item 3.6 of 97/23/EC"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Name","","","","V1","V1","V1"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Current","Recommended fuses","","","A","25","25","25"]
["Notes","","","","","(1) - Nominal water flow rate for Dt: 10°C","(1) - Nominal water flow rate for Dt: 10°C","(1) - Nominal water flow rate for Dt: 10°C"]
["","","","","","(2) - Maximum water flow rate for Dt: 5°C","(2) - Maximum water flow rate for Dt: 5°C","(2) - Maximum water flow rate for Dt: 5°C"]
["","","","","","(3) - Sound levels are measured at: EW 55°C; LW 65°C; Dt 10°C; ambient conditions 7°CDB/6°CWB","(3) - Sound levels are measured at: EW 55°C; LW 65°C; Dt 10°C; ambient conditions 7°CDB/6°CWB","(3) - Sound levels are measured at: EW 55°C; LW 65°C; Dt 10°C; ambient conditions 7°CDB/6°CWB"]
["","","","","","(4) - Sound levels are measured at: EW 70°C; LW 80°C; Dt 10°C; ambient conditions 7°CDB/6°CWB","(4) - Sound levels are measured at: EW 70°C; LW 80°C; Dt 10°C; ambient conditions 7°CDB/6°CWB","(4) - Sound levels are measured at: EW 70°C; LW 80°C; Dt 10°C; ambient conditions 7°CDB/6°CWB"]
["","","","","","(5) - Sound level is valid in free field condition because it is measured in a semi-anechoic room. Measured value under actual installation conditions will be higher due to environmental noise and sound reflections.","(5) - Sound level is valid in free field condition because it is measured in a semi-anechoic room. Measured value under actual installation conditions will be higher due to environmental noise and sound reflections.","(5) - Sound level is valid in free field condition because it is measured in a semi-anechoic room. Measured value under actual installation conditions will be higher due to environmental noise and sound reflections."]
["","","","","","(6) - EW = entering water temperature - LW = leaving water temperature","(6) - EW = entering water temperature - LW = leaving water temperature","(6) - EW = entering water temperature - LW = leaving water temperature"]
["","","","","","(7) - Outdoor ambient, indoor ambient: 5°C~30°C","(7) - Outdoor ambient, indoor ambient: 5°C~30°C","(7) - Outdoor ambient, indoor ambient: 5°C~30°C"]
["","","","","","(8) - For details see operation range TW drawing. In combination EKHBRD* + EMRQ* see EMRQ* operation range! -> -15°C","(8) - For details see operation range TW drawing. In combination EKHBRD* + EMRQ* see EMRQ* operation range! -> -15°C","(8) - For details see operation range TW drawing. In combination EKHBRD* + EMRQ* see EMRQ* operation range! -> -15°C"]
["","","","","","(9) - In accordance with EN/IEC 61000-3-11, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys (system impedance) ≤ Zmax","(9) - In accordance with EN/IEC 61000-3-11, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys (system impedance) ≤ Zmax","(9) - In accordance with EN/IEC 61000-3-11, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys (system impedance) ≤ Zmax"]
["","","","","","(10) - European/International Technical Standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated current ≤ 75A.","(10) - European/International Technical Standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated current ≤ 75A.","(10) - European/International Technical Standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated current ≤ 75A."]
["","","","","","(11) - Zsys: system impedance","(11) - Zsys: system impedance","(11) - Zsys: system impedance"]
["","","","","","(12) - Equipment complying with EN/IEC 61000-3-12","(12) - Equipment complying with EN/IEC 61000-3-12","(12) - Equipment complying with EN/IEC 61000-3-12"]
["","","","","","(13) - European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current larger than 16A and ≤ 75A per phase.","(13) - European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current larger than 16A and ≤ 75A per phase.","(13) - European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current larger than 16A and ≤ 75A per phase."]
["","","","","","(14) - Short-circuit power","(14) - Short-circuit power","(14) - Short-circuit power"]
["","","","","","(15) - Contains fluorinated greenhouse gases","(15) - Contains fluorinated greenhouse gases","(15) - Contains fluorinated greenhouse gases"]