{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHBRD-ADV17"]
[]
[]
[]
[]
["","","","","","EKHBRD011ADV17","EKHBRD014ADV17","EKHBRD016ADV17"]
["Casing","Colour","","","","Metallic grey","Metallic grey","Metallic grey"]
["","Material","","","","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal"]
["Dimensions","Unit","","Height","mm","705","705","705"]
["","","","Width","mm","600","600","600"]
["","","","Depth","mm","695","695","695"]
["Weight","Unit","","","kg","144","144","144"]
["PED","Category","","","","Excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","Excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","Excluded from scope of PED due to article 1, item 3.6 of 97/23/EC"]
["Refrigerant","Type","","","","R-134a","R-134a","R-134a"]
["","Charge","","","kg","2.6","2.6","2.6"]
["Sound power level","Nom.","","","dBA","59","60","60"]
["Sound pressure level","Nom.","","","dBA","43, 46, 0, 0","45, 46, 0, 0","46, 46, 0, 0"]
["Operation range","Heating","Water side","Min.","°C","25","25","25"]
["","","","Max.","°C","80.0","80.0","80.0"]
["Power supply","Name","","","","V1","V1","V1"]
["","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Current","Recommended fuses","","","A","25","25","25"]
["Notes","","","","","(1) - Nominal water flow rate for Dt: 10°C","(1) - Nominal water flow rate for Dt: 10°C","(1) - Nominal water flow rate for Dt: 10°C"]
["","","","","","(2) - Maximum water flow rate for Dt: 5°C","(2) - Maximum water flow rate for Dt: 5°C","(2) - Maximum water flow rate for Dt: 5°C"]
["","","","","","(3) - Sound pressure level is measured in accordance with ISO3744. Sound power level is calculated from sound pressure level.","(3) - Sound pressure level is measured in accordance with ISO3744. Sound power level is calculated from sound pressure level.","(3) - Sound pressure level is measured in accordance with ISO3744. Sound power level is calculated from sound pressure level."]
["","","","","","(4) - Sound levels are measured at: EW 55°C; LW 65°C; Dt 10°C; ambient conditions 7°CDB/6°CWB","(4) - Sound levels are measured at: EW 55°C; LW 65°C; Dt 10°C; ambient conditions 7°CDB/6°CWB","(4) - Sound levels are measured at: EW 55°C; LW 65°C; Dt 10°C; ambient conditions 7°CDB/6°CWB"]
["","","","","","(5) - Sound levels are measured at: EW 70°C; LW 80°C; Dt 10°C; ambient conditions 7°CDB/6°CWB","(5) - Sound levels are measured at: EW 70°C; LW 80°C; Dt 10°C; ambient conditions 7°CDB/6°CWB","(5) - Sound levels are measured at: EW 70°C; LW 80°C; Dt 10°C; ambient conditions 7°CDB/6°CWB"]
["","","","","","(6) - Sound level is valid in free field condition because it is measured in a semi-anechoic room. Measured value under actual installation conditions will be higher due to environmental noise and sound reflections.","(6) - Sound level is valid in free field condition because it is measured in a semi-anechoic room. Measured value under actual installation conditions will be higher due to environmental noise and sound reflections.","(6) - Sound level is valid in free field condition because it is measured in a semi-anechoic room. Measured value under actual installation conditions will be higher due to environmental noise and sound reflections."]
["","","","","","(7) - EW = entering water temperature - LW = leaving water temperature","(7) - EW = entering water temperature - LW = leaving water temperature","(7) - EW = entering water temperature - LW = leaving water temperature"]
["","","","","","(8) - Outdoor ambient, indoor ambient: 5°C~30°C","(8) - Outdoor ambient, indoor ambient: 5°C~30°C","(8) - Outdoor ambient, indoor ambient: 5°C~30°C"]
["","","","","","(9) - For details see operation range TW drawing. In combination EKHBRD* + EMRQ* see EMRQ* operation range! -> -15°C","(9) - For details see operation range TW drawing. In combination EKHBRD* + EMRQ* see EMRQ* operation range! -> -15°C","(9) - For details see operation range TW drawing. In combination EKHBRD* + EMRQ* see EMRQ* operation range! -> -15°C"]