{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSKS-AV3"]
[]
[]
[]
[]
["","","","","","EPSKS04ARV3","EPSKS06ARV3","EPSKS07ARV3"]
["Dimensions","Unit","","Height","mm","958","958","958"]
["","","","Width","mm","1220","1220","1220"]
["","","","Depth","mm","535","535","535"]
["Weight","Unit","","","kg","109","109","109"]
["Fan","Air flow rate","Heating","High","m³/min","78.7","78.7","78.7"]
["","","Cooling","High","m³/min","81.6","81.6","81.6"]
["Operation range","Cooling","","Min.","°CDB","10","10","10"]
["","","","Max.","°CDB","43","43","43"]
["","Domestic hot water","","Min.","°CDB","-28","-28","-28"]
["","","","Max.","°CDB","40","40","40"]
["Sound power level","Heating","","Nom.","dBA","48.2 (1)","48.2 (1)","48.2 (1)"]
["","Cooling","","Nom.","dBA","56.7 (2)","56.7 (2)","56.7 (2)"]
["Sound pressure level","Heating","","Nom.","dBA","29.1 (1)","29.1 (1)","29.1 (1)"]
["","Cooling","","Nom.","dBA","37.3 (2)","37.3 (2)","37.3 (2)"]
["Refrigerant","Type","","","","R-290","R-290","R-290"]
["","GWP","","","","3.0","3.0","3.0"]
["","Charge","","","tCO2Eq","0.0025","0.0025","0.0025"]
["","Charge","","","kg","0.830","0.830","0.830"]
["Piping connections","Level difference","IU - OU","Max.","m","10.0","10.0","10.0"]
["Power supply","Name","","","","V3","V3","V3"]
["","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Current","Recommended fuses","","","A","16","16","25"]
["Notes","","","","","(1) - Measured at LWC 47-55°C ; Ta DB/WB 7°C/6°C.","(1) - Measured at LWC 47-55°C ; Ta DB/WB 7°C/6°C.","(1) - Measured at LWC 47-55°C ; Ta DB/WB 7°C/6°C."]
["","","","","","(2) - Measured at LWC 12-7°C ; Ta 35°C.","(2) - Measured at LWC 12-7°C ; Ta 35°C.","(2) - Measured at LWC 12-7°C ; Ta 35°C."]
["","","","","","(3) - MSC means the maximum current during start up of the compressor","(3) - MSC means the maximum current during start up of the compressor","(3) - MSC means the maximum current during start up of the compressor"]