{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSX07A"]
[]
[]
[]
[]
["","","","","","EPSX07P30AF","EPSX07P50AF"]
["Casing","Colour","","","","Traffic white (RAL9016), Graphite black (RAL9011), Jet black (RAL9005)","Traffic white (RAL9016), Graphite black (RAL9011), Jet black (RAL9005)"]
["","Material","","","","Impact resistant polypropylene","Impact resistant polypropylene"]
["Dimensions","Unit","","Height","mm","1914","1906"]
["","","","Width","mm","590","785"]
["","","","Depth","mm","671","837"]
["Weight","Unit","","","kg","84.0","105"]
["PED","Category","","","","Art4.3","Art4.3"]
["Sound power level","Nom.","","","dBA","47.0","47.0"]
["Sound pressure level","Nom.","","","dBA","24.8","24.8"]
["Operation range","Heating","Water side","Min.","°C","0 (3)","0 (3)"]
["","","","Max.","°C","0 (3)","0 (3)"]
["","Cooling","Ambient","Min.","°CDB","0 (3)","0 (3)"]
["","","Water side","Min.","°C","0 (3)","0 (3)"]
["","","","Max.","°C","0 (3)","0 (3)"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","230","230"]
["Electric heater","Power supply","","Name","","6V / 9W","6V / 9W"]
["","","","Phase","","1~ / 3~","1~ / 3~"]
["","","","Frequency","Hz","50","50"]
["","","","Voltage","V","230/400","230/400"]
["","Recommended fuses","","","A","0.000 (4)","0.000 (4)"]
["Notes","","","","","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897"]
["","","","","","(2) - Minimum required volume, excluding the volume in the unit","(2) - Minimum required volume, excluding the volume in the unit"]
["","","","","","(3) - Refer to drawing operation limits","(3) - Refer to drawing operation limits"]
["","","","","","(4) - Refer to wiring diagram and installation manual for correct recommended fuse depending on power supply and grid connection","(4) - Refer to wiring diagram and installation manual for correct recommended fuse depending on power supply and grid connection"]