{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":11,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPVX07UA / EPSKS-AV3"]
[]
[]
[]
[]
["","","","","","EPVX07SU18AJ4V / EPSKS04ARV3","EPVX07SU23AJ4V / EPSKS04ARV3","EPVX07SU18AJ4V / EPSKS06ARV3","EPVX07SU23AJ4V / EPSKS06ARV3","EPVX07SU18AJ4V / EPSKS07ARV3","EPVX07SU23AJ4V / EPSKS07ARV3"]
["Indoor unit","","","","","EPVX07S18AJ4V","EPVX07S23AJ4V","EPVX07S18AJ4V","EPVX07S23AJ4V","EPVX07S18AJ4V","EPVX07S23AJ4V"]
["Heating capacity","Nom.","","","kW","5.25 (1)","5.25 (1)","5.25 (1)","5.25 (1)","5.25 (1)","5.25 (1)"]
["Cooling capacity","Nom.","","","kW","5.16 (2), 6.71 (3)","5.16 (2), 6.71 (3)","5.16 (2), 6.71 (3)","5.16 (2), 6.71 (3)","5.16 (2), 6.71 (3)","5.16 (2), 6.71 (3)"]
["Power input","Heating","","Nom.","kW","1.02 (1)","1.02 (1)","1.02 (1)","1.02 (1)","1.02 (1)","1.02 (1)"]
["","Cooling","","Nom.","kW","1.71 (2), 1.62 (3)","1.71 (2), 1.62 (3)","1.71 (2), 1.62 (3)","1.71 (2), 1.62 (3)","1.71 (2), 1.62 (3)","1.71 (2), 1.62 (3)"]
["","Domestic hot water from 10°C to 50°C","","Nom.","kWh","2.19","2.50","2.19","2.50","2.19","2.50"]
["Heat up time from 10°C to 50°C","hr","","","","2h 01min","2h 23min","2h 01min","2h 23min","2h 01min","2h 23min"]
["COP","","","","","5.17 (1)","5.17 (1)","5.17 (1)","5.17 (1)","5.17 (1)","5.17 (1)"]
["EER","","","","","3.01 (2), 6.71 (3)","3.01 (2), 6.71 (3)","3.01 (2), 6.71 (3)","3.01 (2), 6.71 (3)","3.01 (2), 6.71 (3)","3.01 (2), 6.71 (3)"]
["Domestic hot water heating","General","","Declared load profile","","L","L","L","L","L","L"]
["","Average climate","","Water heating energy efficiency class","","A+","A+","A+","A+","A+","A+"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.69","3.69","3.81","3.81","3.83","3.83"]
["","","","Seasonal space heating eff. class","","A++","A++","A+++","A+++","A+++","A+++"]
["","Average climate water outlet 35°C","General","SCOP","","5.03","5.03","5.05","5.05","5.05","5.05"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Notes","","","","","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]