{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPVX10UA4V / EPSK06-10AV3"]
[]
[]
[]
[]
["","","","","","EPVX10SU18AJ4V / EPSK06ARV3","EPVX10SU23AJ4V / EPSK06ARV3","EPVX10SU18AJ4V / EPSK08ARV3","EPVX10SU23AJ4V / EPSK08ARV3","EPVX10SU18AJ4V / EPSK10ARV3","EPVX10SU23AJ4V / EPSK10ARV3"]
["Heating capacity","Nom.","","","kW","5.81 (1)","5.81 (1)","7.62 (1)","7.62 (1)","8.11 (1)","8.11 (1)"]
["Cooling capacity","Nom.","","","kW","6.00 (2), 6.37 (3)","6.00 (2), 6.37 (3)","6.89 (2), 6.37 (3)","6.89 (2), 6.37 (3)","7.84 (2), 6.37 (3)","7.84 (2), 6.37 (3)"]
["Power input","Heating","","Nom.","kW","1.12 (1)","1.12 (1)","1.52 (1)","1.52 (1)","1.64 (1)","1.64 (1)"]
["","Cooling","","Nom.","kW","1.55 (2), 1.13 (3)","1.55 (2), 1.13 (3)","1.85 (2), 1.13 (3)","1.85 (2), 1.13 (3)","2.17 (2), 1.13 (3)","2.17 (2), 1.13 (3)"]
["","Domestic hot water from 10°C to 50°C","","Nom.","kWh","2.35","2.89","2.35","2.89","2.35","2.89"]
["Heat up time from 10°C to 50°C","hr","","","","1h 27min","1h 58min","1h 27min","1h 58min","1h 27min","1h 58min"]
["COP","","","","","5.19 (1)","5.19 (1)","5.01 (1)","5.01 (1)","4.94 (1)","4.94 (1)"]
["EER","","","","","3.87 (2), 5.63 (3)","3.87 (2), 5.63 (3)","3.73 (2), 5.63 (3)","3.73 (2), 5.63 (3)","3.62 (2), 5.63 (3)","3.62 (2), 5.63 (3)"]
["Domestic hot water heating","General","","Declared load profile","","L","L","L","L","L","L"]
["","Average climate","","Water heating energy efficiency class","","A+","A+","A+","A+","A+","A+"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.91","3.91","3.97","3.97","4.02","4.02"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++","A+++","A+++"]
["","Average climate water outlet 35°C","General","SCOP","","5.12","5.12","5.15","5.15","5.15","5.15"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Notes","","","","","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]