{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLA-DW17"]
[]
[]
[]
[]
["","","","","","ERLA16D2W17","ERLA16DAW17"]
["Dimensions","Unit","","Height","mm","870","870"]
["","","","Width","mm","1,100","1,100"]
["","","","Depth","mm","460","460"]
["Weight","Unit","","","kg","101","101"]
["Fan","Air flow rate","Heating","High","m³/min","85.0","85.0"]
["","","Cooling","High","m³/min","85","85"]
["Operation range","Cooling","","Min.","°CDB","10","10"]
["","","","Max.","°CDB","43","43"]
["","Domestic hot water","","Min.","°CDB","-25","-25"]
["","","","Max.","°CDB","25 (1), 35 (1)","25 (1), 35 (1)"]
["Sound power level","Heating","","Nom.","dBA","62.0 (2)","62.0 (2)"]
["Sound pressure level","Heating","","Nom.","dBA","48.0 (2)","48.0 (2)"]
["Refrigerant","Type","","","","R-32","R-32"]
["","GWP","","","","675.0","675.0"]
["","Charge","","","tCO2Eq","2.57","2.57"]
["","Charge","","","kg","3.8","3.8"]
["Piping connections","Liquid","","OD","mm","9.5","9.5"]
["","Gas","","OD","mm","15.9","15.9"]
["","Drain","","OD","mm","26","26"]
["","Level difference","IU - OU","Max.","m","30.0","30.0"]
["","Heat insulation","","","","Both liquid and gas pipes","Both liquid and gas pipes"]
["Power supply","Name","","","","W1","W1"]
["","Phase","","","","3~","3~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","400","400"]
["Current","Recommended fuses","","","A","16","16"]
["Notes","","","","","(1) - For more details, see operation range drawing","(1) - For more details, see operation range drawing"]
["","","","","","(2) - Measured with a pressure drop of 10 kPa in the heating system at an operating condition of leaving water 47-55°C in a room with an ambient of 20°C. DB/WB 7°C/6°.","(2) - Measured with a pressure drop of 10 kPa in the heating system at an operating condition of leaving water 47-55°C in a room with an ambient of 20°C. DB/WB 7°C/6°."]