{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":11,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETBX-D9W / EPRA014-018DV"]
[]
[]
[]
[]
["","","","","","ETBX16DA9W / EPRA14DAV3","ETBX16DF9W / EPRA14DAV3","ETBX16DA9W / EPRA16DAV3","ETBX16DF9W / EPRA16DAV3","ETBX16DA9W / EPRA18DAV3","ETBX16DF9W / EPRA18DAV3"]
["COP","","","","","4.67","4.67","5.00 (2)","5.00","5.00","5.00"]
["Indoor unit","","","","","ETBX16DA9W","ETBX16DA9W","ETBX16DA9W","ETBX16DA9W","ETBX16DA9W","ETBX16DA9W"]
["Space heating","Average climate water outlet 35°C","General","ηs (Seasonal space heating efficiency)","%","","","180"]
["","","","Seasonal space heating eff. class","","","","A+++"]
["","","","SCOP","","","","4.57"]
["","Average climate water outlet 55°C","General","Seasonal space heating eff. class","","","","A++"]
["","","","ηs (Seasonal space heating efficiency)","%","","","142"]
["","","","SCOP","","","","3.62"]
["Cooling capacity","Nom.","","","kW","","","11.5 (3), 7.88 (4)"]
["EER","","","","","4.13, 2.70","4.13, 2.70","4.11 (3), 2.69 (4)","4.11, 2.69","4.09, 2.68","4.09, 2.68"]
["Heating capacity","Nom.","","","kW","","","9.00 (2)"]
["","Min.","","","kW","","","3.96 (1)"]
["","Max.","","","kW","","","10.91 (1)"]
["Power input","Heating","","Max.","kW","","","2.24 (5)"]
["","","","Min.","kW","","","0.95 (5)"]
["","","","Nom.","kW","","","1.80 (2)"]
["","Cooling","","Nom.","kW","","","2.80 (3), 2.93 (4)"]
["Notes","","","","","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]
["","","","","","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511"]
["","","","","","(6) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(6) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(6) - Test at Ta DB/WB 7°C/6°C. According to EN 16147.","(6) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(6) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(6) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed"]
["","","","","","","","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed"]
["Heating capacity","Min.","","","kW","3.70","3.70","","3.96","4.40","4.40"]
["","Nom.","","","kW","5.69","5.69","","9.00","9.00","9.00"]
["","Max.","","","kW","10.18","10.18","","10.91","12.12","12.12"]
["Cooling capacity","Nom.","","","kW","10.6, 6.90","10.6, 6.90","","11.5, 7.88","12.5, 8.86","12.5, 8.86"]
["Power input","Heating","","Min.","kW","0.88","0.88","","0.95","1.05","1.05"]
["","","","Nom.","kW","1.22","1.22","","1.80","1.80","1.80"]
["","","","Max.","kW","2.09","2.09","","2.24","2.49","2.49"]
["","Cooling","","Nom.","kW","2.55, 2.56","2.55, 2.56","","2.80, 2.93","3.05, 3.31","3.05, 3.31"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.62","3.62","","3.62","3.62","3.62"]
["","","","Seasonal space heating eff. class","","A++","A++","","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.57","4.57","","4.57","4.57","4.57"]
["","","","Seasonal space heating eff. class","","A+++","A+++","","A+++","A+++","A+++"]