{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSX16E7"]
[]
[]
[]
[]
["","","","","","ETSX16P30EF7","ETSX16P30EG7","ETSX16P50EF7","ETSX16P50EG7"]
["Casing","Colour","","","","Traffic white (RAL9016) / Traffic black (RAL9017)","Traffic white (RAL9016) / Traffic black (RAL9017)","Traffic white (RAL9016) / Traffic black (RAL9017)","Traffic white (RAL9016) / Traffic black (RAL9017)"]
["","Material","","","","Impact resistant polypropylene","Impact resistant polypropylene","Impact resistant polypropylene","Impact resistant polypropylene"]
["Dimensions","Unit","","Height","mm","1892","1892","1910","1910"]
["","","","Width","mm","594","594","792","792"]
["","","","Depth","mm","644","644","816","817"]
["Weight","Unit","","","kg","75","75","98","98"]
["Sound power level","Nom.","","","dBA","45.6","45.6","45.6","45.6"]
["Sound pressure level","Nom.","","","dBA","32.8","32.8","32.8","32.8"]
["Operation range","Heating","Water side","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","Cooling","Ambient","Min.","°CDB","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","Water side","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)","0 (2)","0 (2)"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","230","230","230","230"]
["Notes","","","","","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897","(1) - Heatloss according to EN12897"]
["","","","","","(2) - Refer to operation limits drawings","(2) - Refer to operation limits drawings","(2) - Refer to operation limits drawings","(2) - Refer to operation limits drawings"]