{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":11,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSXB16E / EPRA14-18DW7"]
[]
[]
[]
[]
["","","","","","ETSXB16P30EF / EPRA14DAW17","ETSXB16P50EF / EPRA14DAW17","ETSXB16P50EF / EPRA16DAW17","ETSXB16P30EF / EPRA16DAW17","ETSXB16P50EF / EPRA18DAW17","ETSXB16P30EF / EPRA18DAW17"]
["Heating capacity","Min.","","","kW","","","396.00 (1)","396.00 (1)"]
["","Nom.","","","kW","","","9.00 (2)","9.00 (2)"]
["","Max.","","","kW","","","1,044.00 (1)","1,044.00 (1)"]
["Cooling capacity","Nom.","","","kW","","","115 (3), 788 (4)","115 (3), 788 (4)"]
["Power input","Heating","","Min.","kW","","","9.00 (5)","9.00 (5)"]
["","","","Nom.","kW","","","18.0 (2)","18.0 (2)"]
["","","","Max.","kW","","","232.00 (5)","232.00 (5)"]
["","Cooling","","Nom.","kW","","","28.0 (3), 293 (4)","28.0 (3), 293 (4)"]
["COP","","","","","479.00","479.00","5.00 (2)","5.00 (2)","5.00","5.00"]
["EER","","","","","413.00, 27.00","413.00, 27.00","411.00 (3), 269.00 (4)","411.00 (3), 269.00 (4)","409.00, 268.00","409.00, 268.00"]
["Domestic hot water heating","General","","Declared load profile","","","","XL","L"]
["","Average climate","","Water heating energy efficiency class","","","","A+","A+"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","","","3.63","3.63"]
["","","","Seasonal space heating eff. class","","","","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","","","4.81","4.81"]
["","","","Seasonal space heating eff. class","","","","A+++","A+++"]
["Notes","","","","","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]
["","","","","","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(4) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(5) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511"]
["Heating capacity","Min.","","","kW","37.00","37.00","","","44.00","44.00"]
["","Nom.","","","kW","59.0","59.0","","","9.00","9.00"]
["","Max.","","","kW","975.00","975.00","","","116.00","116.00"]
["Cooling capacity","Nom.","","","kW","106, 69.0","106, 69.0","","","125, 886","125, 886"]
["Power input","Heating","","Min.","kW","84.00","84.00","","","1.00","1.00"]
["","","","Nom.","kW","123","123","","","18.0","18.0"]
["","","","Max.","kW","217.00","217.00","","","258.00","258.00"]
["","Cooling","","Nom.","kW","255, 256","255, 256","","","305, 331","305, 331"]
["Domestic hot water heating","General","","Declared load profile","","L","XL","","","XL","L"]
["","Average climate","","Water heating energy efficiency class","","A+","A+","","","A+","A+"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.63","3.63","","","3.63","3.63"]
["","","","Seasonal space heating eff. class","","A++","A++","","","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.81","4.81","","","4.81","4.81"]
["","","","Seasonal space heating eff. class","","A+++","A+++","","","A+++","A+++"]