{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-A / ARXM-R"]
[]
[]
[]
[]
["","","","","FAA71AUVEB / ARXM71R2V1B","FAA71AUVEB / ARXM71R5V1B"]
["Cooling capacity","Max.","","kW","6.95","6.95"]
["","Nom.","","kW","6.80","6.80"]
["Space cooling","SEER","","","5.77","5.77"]
["","Annual energy consumption","","kWh/a","412","412"]
["","Capacity","Pdesign","kW","6.80","6.80"]
["","Energy efficiency class","","","A+","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.50","4.50"]
["","SCOP/A","","","3.81","3.81"]
["","Energy efficiency class","","","A","A"]
["","Pdh Heating capacity at -10°","","kW","4.50","4.50"]
["","Annual energy consumption","","kWh/a","1,652","1,652"]
["Nominal efficiency","Annual energy consumption","","kWh","1,000","1,000"]
["","EER","","","3.40","3.40"]
["","COP","","","3.19","3.19"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","D","D"]
["Heating capacity","Nom.","","kW","7.50","7.50"]
["","Max.","","kW","7.59","7.59"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]