{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":7,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-A"]
[]
[]
[]
[]
["","","","","","FAA71AUVEB","FAA100AUVEB"]
["Casing","Colour","","","","Fresh White","Fresh White"]
["","Material","","","","Resin","Resin"]
["Dimensions","Unit","","Height","mm","290","340"]
["","","","Width","mm","1050","1200"]
["","","","Depth","mm","238","240"]
["Weight","Unit","","","kg","13.0","17.0"]
["Fan","Air flow rate","Cooling","High","m³/min","18.0","26.0"]
["","","","Medium","m³/min","16","23"]
["","","","Low","m³/min","14.0","19.0"]
["","","Heating","High","m³/min","18.0","26.0"]
["","","","Medium","m³/min","16.0","23.0"]
["","","","Low","m³/min","14.0","19.0"]
["Sound power level","Cooling","","","dBA","61","65"]
["","Heating","","","dBA","61","65"]
["Sound pressure level","Cooling","","High","dBA","45","49"]
["","","","Medium","dBA","42","45"]
["","","","Low","dBA","40","41"]
["","Heating","","High","dBA","45","49"]
["","","","Medium","dBA","42","45"]
["","","","Low","dBA","40","41"]
["Piping connections","Liquid","","OD","mm","9.52","9.52"]
["","Gas","","OD","mm","15.9","15.9"]
["","Drain","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Control systems","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]