{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":20,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RZAG-MV1"]
[]
[]
[]
[]
["","","","","FBA100A2VEB / RZAG100M7V1B","FBA100A2VEB / RZAG71M7V1B","FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / RZAG100M7V1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZAG71M7V1B","FBA35A2VEB9 / FBA35A2VEB9 / RZAG71M7V1B","FBA50A2VEB9 / FBA50A2VEB9 / RZAG71M7V1B","FBA71A2VEB9 / RZAG71M7V1B","FBA140A2VEB / RZAG100M7V1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZAG100M7V1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZAG100M7V1B","FBA50A2VEB9 / FBA50A2VEB9 / RZAG100M7V1B","FBA71A2VEB9 / FBA71A2VEB9 / RZAG100M7V1B","FBA125A2VEB / RZAG125M7V1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZAG125M7V1B","FBA140A2VEB / RZAG140M7V1B","FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / FBA35A2VEB9 / RZAG140M7V1B"]
["Cooling capacity","Nom.","","kW","","","","6.80 (1)","6.80 (1)","6.80 (1)","6.80 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","12.1 (1)","12.1 (1)","13.4 (1)","13.4 (1)"]
["Space cooling","SEER","","","","","","5.08","5.94","5.45","6.22","6.39","5.81","5.86","6.52","7.88","6.19","11.2","6.42","11.5"]
["","Annual energy consumption","","kWh/a","","","","469","401","437","382","520","572","567","510","422","1,173","649","1,252","699"]
["","Capacity","Pdesign","kW","","","","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","12.1","12.1","13.4","13.4"]
["","Energy efficiency class","","","","","","B","A+","A","A++","A++","A+","A+","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","","","4.70","4.70","4.70","4.70","7.80","7.80","7.80","7.80","7.80","9.52","9.52","9.52","9.52"]
["","SCOP/A","","","","","","3.80","3.87","3.88","4.20","4.20","3.92","4.00","4.12","4.43","4.12","5.95","4.11","4.00"]
["","Energy efficiency class","","","","","","A","A","A","A+","A+","A","A","A+","A+"]
["","Annual energy consumption","","kWh/a","","","","1,732","1,700","1,696","1,566","2,600","2,786","2,730","2,651","2,465","3,235","2,240","3,243","3,332"]
["Heating capacity","Nom.","","kW","","","","7.50 (2)","7.50 (2)","7.50 (2)","7.50 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","13.5 (2)","13.5 (2)","15.5 (2)","15.5 (2)"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notes","","","","","","","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","","","","(3) - See separate drawing for operation range","","(3) - See separate drawing for operation range","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","","","","","(4) - See separate drawing for electrical data","","(4) - See separate drawing for electrical data","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]