{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":5,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / RZASG-MY1"]
[]
[]
[]
[]
["","","","","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZASG140M7Y1B"]
["Outdoor unit","","","","RZASG140M7Y1B"]
["Cooling capacity","Nom.","","kW","13.4"]
["Heating capacity","Nom.","","kW","15.5"]
["Space cooling","Capacity","Pdesign","kW","13.4"]
["","SEER","","","9.67"]
["","Annual energy consumption","","kWh/a","832"]
["Space heating (Average climate)","Capacity","Pdesign","kW","7.80"]
["","SCOP/A","","","5.62"]
["","Annual energy consumption","","kWh/a","1943"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]