{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RXS-L"]
[]
[]
[]
[]
["","","","","FBQ50D2VEB / RXS50L2V1B","FBQ60D2VEB / RXS60L2V1B"]
["Cooling capacity","Nom.","","kW","5.0 (2)","5.7 (2)"]
["Space cooling","SEER","","","6.21","5.86"]
["","Annual energy consumption","","kWh/a","282","340"]
["","Capacity","Pdesign","kW","5.00","5.70"]
["","Energy efficiency class","","","A++","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.40","4.60"]
["","SCOP/A","","","4.06","4.01"]
["","Energy efficiency class","","","A+","A+"]
["","Annual energy consumption","","kWh/a","1,517","1,606"]
["Nominal efficiency","Annual energy consumption","","kWh","710","826"]
["","EER","","","3.52 (1)","3.45 (1)"]
["","COP","","","3.83 (1)","3.71 (1)"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Heating capacity","Nom.","","kW","5.50 (2)","7.00 (2)"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]