{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":5,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / ARXM-N9"]
[]
[]
[]
[]
["","","","","FCAG71BVEB / ARXM71N2V1B9"]
["Cooling capacity","Nom.","","kW","6.80"]
["","Max.","","kW","7.05"]
["Heating capacity","Nom.","","kW","7.50"]
["","Max.","","kW","7.58"]
["Nominal efficiency","Annual energy consumption","","kWh","1,083"]
["","COP","","","3.38"]
["","EER","","","3.14"]
["","Energy labeling Directive","Cooling","","B"]
["","","Heating","","C"]
["Space cooling","Annual energy consumption","","kWh/a","405"]
["","Energy efficiency class","","","A+"]
["","Capacity","Pdesign","kW","6.80"]
["","SEER","","","5.87"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","1,573"]
["","Capacity","Pdesign","kW","4.50"]
["","Energy efficiency class","","","A+"]
["","Pdh Heating capacity at -10°","","kW","4.50"]
["","SCOP/A","","","4.00"]
["Notes","","","","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data"]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]