{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":23,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100BVEB / RZQG100L8Y1B","FCAG71BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG100BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG140BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG100L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG125BVEB / RZQG125L8Y1B","FCAG60BVEB / FCAG60BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG125L8Y1B","FCAG140BVEB / RZQG125L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG125L8Y1B","FCAG140BVEB / RZQG140L7Y1B"]
["Energy Efficiency Range","","","","A+++ ~ D"]
["Cooling capacity","Nom.","","kW","","6.80","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00","12.00","12.00","13.40"]
["Heating capacity","Nom.","","kW","","7.50","","","","","","","","","","","13.50","","","","","","15.50"]
["Nominal efficiency","EER","","","","3.39","3.30","3.30","3.30","3.39","3.81","3.87","3.75","3.75","3.75","3.11","3.71","3.61","3.73","3.71","3.61","3.61","2.50"]
["","COP","","","","3.97","","","","","","","","","","","3.63","","","","","","3.61"]
["","Annual energy consumption","","kWh","","1,003","","","","","","","","","","","1,617"]
["","Energy labeling Directive","Cooling","","","A","","","","","","","","","","","A"]
["","","Heating","","","A","","","","","","","","","","","A"]
["Space cooling","Energy efficiency class","","","","A++","A","A","A","A++","A","A++","A","A","A","A","A+","A","A","A+","A","A"]
["","Capacity","Pdesign","kW","","6.80","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00","12.00","12.00","13.40"]
["","SEER","","","","6.72","5.10","5.10","5.10","6.80","5.10","6.80","5.10","5.10","5.10","5.10","6.00","5.10","5.10","6.00","5.10","5.10","6.44"]
["","Annual energy consumption","","kWh/a","","355","467","467","467","350","652","489","652","652","652","652","700","824","824","700","824","824","1,249"]
["Space heating (Average climate)","Energy efficiency class","","","","A+","A","A","A","A+","A","A++","A","A","A","A","A+","A","A","A+","A","A"]
["","Capacity","Pdesign","kW","","6.33","6.00","6.00","6.00","6.33","11.30","11.30","11.30","11.30","11.30","7.60","12.66","12.71","12.71","12.66","12.71","12.71","11.56"]
["","SCOP/A","","","","4.20","3.80","3.80","3.80","4.20","3.80","4.61","3.80","3.80","3.80","3.81","4.10","3.80","3.80","4.10","3.80","3.80","4.27"]
["","Annual energy consumption","","kWh/a","","2,110","2,211","2,211","2,211","2,110","4,164","3,432","4,164","4,164","4,164","2,790","4,323","4,683","4,683","4,323","4,683","4,683","3,795"]
["Notes","","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","","","","(3) - See separate drawing for operation range","","","(3) - See separate drawing for operation range","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","","","","(4) - See separate drawing for electrical data","","","(4) - See separate drawing for electrical data","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]