{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":11,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RZAG-MY1"]
[]
[]
[]
[]
["","","","","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZAG71M7Y1B","FDXM35F3V1B / FDXM35F3V1B / RZAG71M7Y1B","FDXM50F3V1B / FDXM50F3V1B / RZAG71M7Y1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZAG100M7Y1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZAG100M7Y1B","FDXM50F3V1B / FDXM50F3V1B / FDXM50F3V1B / RZAG100M7Y1B","FDXM50F3V1B / FDXM50F3V1B / RZAG100M7Y1B"]
["Cooling capacity","Nom.","","kW","6.80 (1)","6.80 (1)","","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)"]
["Space cooling","Annual energy consumption","","kWh/a","377","380","","416","423","379","387"]
["","Capacity","Pdesign","kW","6.80","6.80","","9.50","9.50","9.50","9.50"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.70","4.70","","7.80","7.80","7.80","7.80"]
["","Annual energy consumption","","kWh/a","1,537","1,589","","2,438","2,540","2,324","2,421"]
["Heating capacity","Nom.","","kW","7.50 (2)","7.50 (2)","","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)"]
["Space cooling","SEER","","","6.32","6.27","","8.00","7.86","8.77","8.60"]
["","Energy efficiency class","","","A++","A++","","A++","A++","A+++","A+++"]
["Space heating (Average climate)","SCOP/A","","","4.28","4.14","","4.48","4.30","4.70","4.51"]
["","Energy efficiency class","","","A+","A+","","A+","A+","A++","A+"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Outdoor unit","","","","","","RZAG71M7Y1B"]
["Cooling capacity","Nom.","","kW","","","6.80"]
["Heating capacity","Nom.","","kW","","","7.50"]
["Space cooling","Energy efficiency class","","","","","A++"]
["","Capacity","Pdesign","kW","","","6.80"]
["","SEER","","","","","7.12"]
["","Annual energy consumption","","kWh/a","","","334"]
["Space heating (Average climate)","Energy efficiency class","","","","","A+"]
["","Capacity","Pdesign","kW","","","4.70"]
["","SCOP/A","","","","","4.43"]
["","Annual energy consumption","","kWh/a","","","1485"]
["Energy Efficiency Range","","","","","","A+++ ~ D"]