{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":7,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-A9"]
[]
[]
[]
[]
["","","","","FFA25A2VEB9 / RXM25A5V1B9","FFA35A2VEB9 / RXM35A5V1B9","FFA50A2VEB9 / RXM50A5V1B9"]
["Cooling capacity","Nom.","","kW","2.5","3.4","5"]
["Heating capacity","Nom.","","kW","3.2","4.2","5.8"]
["Nominal efficiency","EER","","","4.57","3.81","3.24"]
["","COP","","","3.9","3.5","3.49"]
["","Annual energy consumption","","kWh","274","446","772"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","A","B","B"]
["Space cooling","Energy efficiency class","","","A++","A++","A+"]
["","Capacity","Pdesign","kW","2.5","3.4","5"]
["","SEER","","","6.32","6.47","5.98"]
["","Annual energy consumption","","kWh/a","138","184","293"]
["Space heating (Average climate)","Energy efficiency class","","","A+","A+","A"]
["","Capacity","Pdesign","kW","2.31","3.1","3.84"]
["","SCOP/A","","","4.29","4.19","3.9"]
["","Pdh Heating capacity at -10°","","kW","1.84","2.5","3.4"]
["","Annual energy consumption","","kWh/a","754","1035","1378"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - See separate drawing for operation range"]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - See separate drawing for electrical data"]