{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":9,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Casing","Colour","","","","White","White","White","White"]
["","Material","","","","Resin, sheet metal","Resin, sheet metal","Resin, sheet metal","Resin, sheet metal"]
["Dimensions","Unit","","Height","mm","235","235","235","235"]
["","","","Width","mm","960","960","1270","1270"]
["","","","Depth","mm","690","690","690","690"]
["Weight","Unit","","","kg","24.0","25.0","31.0","32.0"]
["Fan","Air flow rate","Cooling","High","m³/min","14.0","15.0","19.5","20.5"]
["","","","Medium","m³/min","11.5","12.0","15.0","17.0"]
["","","","Low","m³/min","10.0","10.0","11.5","14.0"]
["","","Heating","High","m³/min","14.0","15.0","19.5","20.5"]
["","","","Medium","m³/min","11.5","12.0","15.0","17.0"]
["","","","Low","m³/min","10.0","10.0","11.5","14.0"]
["Sound power level","Cooling","","","dBA","53","54","54","55"]
["Sound pressure level","Cooling","","High","dBA","36","37","37","38"]
["","","","Medium","dBA","34","35","35","36"]
["","","","Low","dBA","31","32","33","34"]
["","Heating","","High","dBA","36","37","37","38"]
["","","","Medium","dBA","31","32","33","34"]
["","","","Nom.","dBA","34","35","35","36"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","9.52"]
["","Gas","","OD","mm","9.50","12.7","12.7","15.9"]
["","Drain","","","","VP20","VP20","VP20","VP20"]
["Control systems","Infrared remote control","","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["","Wired remote control","","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["Standard Accessories","Thermal insulation tube","","","","2","2","2","2"]
["","Resin bushing","","","","1","1","1","1"]
["","Wiring fixture","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Wire clamp material","","","","7","7","7","7"]
["","Drain hose","","","","1","1","1","1"]
["","Screws","","","","2","2","2","2"]
["","Sealing pad (large)","","","","1","1","1","1"]
["","Sealing pad (small)","","","","1","1","1","1"]
["","Washer","","","","8","8","8","8"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data"]