{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":62,"n_cols":8,"rows_kept":62,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B"]
[]
[]
[]
[]
["","","","","","FLXS25BAVMB","FLXS50BAVMB","FLXS60BAVMB"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","7.6","11.4","10.7"]
["Sound pressure level","Cooling","","Nom.","dBA","34","43","45"]
["Fan","Air flow rate","Heating","Nom.","m³/min","8.3","9.8","10.6"]
["Sound pressure level","Heating","","Nom.","dBA","34","41","42"]
["Casing","Colour","","","","Almond white","Almond white","Almond white"]
["Dimensions","Unit","","Height","mm","490","490","490"]
["","","","Width","mm","1050","1050","1050"]
["","","","Depth","mm","200","200","200"]
["Weight","Unit","","","kg","16","17","17"]
["Fan","Air flow rate","Cooling","High","m³/min","7.6","11.4","12.0"]
["","","","Medium","m³/min","","","10.7"]
["","","","Low","m³/min","6","8.5","9.3"]
["","","","Silent operation","m³/min","5.2","7.5","8.3"]
["","","Heating","High","m³/min","9.2","12.1","12.8"]
["","","","Medium","m³/min","","","10.6"]
["","","","Low","m³/min","7.4","7.5","8.4"]
["","","","Silent operation","m³/min","6.6","6.8","7.5"]
["Sound power level","Cooling","","","dBA","51","60","60"]
["","Heating","","","dBA","51","","59"]
["Sound pressure level","Cooling","","High","dBA","37","47","48"]
["","","","Medium","dBA","","","45"]
["","","","Low","dBA","31","39","41"]
["","","","Silent operation","dBA","28","36","39"]
["","Heating","","High","dBA","37","46","47"]
["","","","Medium","dBA","","","42"]
["","","","Low","dBA","31","35","37"]
["","","","Silent operation","dBA","29","33","34"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.52","12.7","12.7"]
["","Drain","","","","18","18","18"]
["Control systems","Infrared remote control","","","","ARC433B67","ARC433B67","ARC433B67"]
["Standard Accessories","Air purification filter","","","","1","1","1"]
["","Binding band","","","","4","4","4"]
["","Batteries","","","","2","2","2"]
["","Heat insulation tube (refrigerant pipe)","","","","1","2"]
["","Infrared remote control","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Photocatalytic deodorizing filter","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["","Side cover","","","","2","2","2"]
["Power supply","Name","","","","VM","VM","V1"]
["","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50/60","50/60","50"]
["","Voltage","","","V","220-240/220-230","220-240/220-230","230"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - SL: The silent fan level of the air flow rate setting"]
["","","","","","(2) - 230V","(2) - 230V","(2) - For cooling/heating capacity, maximum interunit piping length and maximum installation height difference, please refer to the specifications of the outdoor unit to be connected."]
["","","","","","(3) - 240V","(3) - 240V","(3) - Contains fluorinated greenhouse gases"]
["","","","","","(4) - Sound values are measured in an anechoic room.","(4) - Sound values are measured in an anechoic room.","(4) - Electric characteristics are only for fan coil unit."]
["","","","","","(5) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(5) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","","(6) - The sound power level is an absolute value indicating the power which a sound source generates.","(6) - The sound power level is an absolute value indicating the power which a sound source generates."]
["Standard Accessories","Extension auxiliary pipe","","","","","2","2"]
["","Installation manual","","","","","","1"]
["","Wireless remote control","","","","","","1"]
["","Operation manual","","","","","","1"]
["","Heat insulating tape","","","","","","2"]