{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":7,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B"]
[]
[]
[]
[]
["","","","","FLXS25BAVMB","FLXS50BAVMB","FLXS60BAVMB"]
["Sound pressure level","Heating","High","dBA","37","46","47"]
["","","Medium","dBA","","","42"]
["","","Silent operation","dBA","29","33","34"]
["","","Low","dBA","31","35","37"]
["","Cooling","Medium","dBA","","","45"]
["","","Silent operation","dBA","28","36","39"]
["","","Low","dBA","31","39","41"]
["","","High","dBA","37","47","48"]
["","","Nom.","dBA","34","41","42"]
["","Cooling","Nom.","dBA","34","43","45"]
["Standard Accessories","Installation and operation manual","","","1","1"]
["","Infrared remote control","","","1","1"]
["","Batteries","","","2","2","2"]
["","Remote control holder","","","1","1","1"]
["","Air purification filter","","","1","1","1"]
["","Heat insulation tube (refrigerant pipe)","","","1","2"]
["","Mounting plate","","","1","1","1"]
["","Side cover","","","2","2","2"]
["","Binding band","","","4","4","4"]
["","Photocatalytic deodorizing filter","","","1","1","1"]
["Control systems","Infrared remote control","","","ARC433B67","ARC433B67","ARC433B67"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gas","OD","mm","9.52","12.7","12.7"]
["","Drain","","","18","18","18"]
["Sound power level","Cooling","","dBA","51","60","60"]
["","Heating","","dBA","51","","59"]
["Dimensions","Unit","Width","mm","1,050","1,050","1,050"]
["","","Depth","mm","200","200","200"]
["","","Height","mm","490","490","490"]
["Casing","Colour","","","Almond white","Almond white","Almond white"]
["Weight","Unit","","kg","16","17","17"]
["Power supply","Phase","","","1~","1~","1~"]
["","Name","","","VM","VM","V1"]
["","Frequency","","Hz","50/60","50/60","50"]
["","Voltage","","V","220-240/220-230","220-240/220-230","230"]
["Notes","","","","(1) - 220V","(1) - 220V","(1) - SL: The silent fan level of the air flow rate setting"]
["","","","","(2) - 230V","(2) - 230V","(2) - For cooling/heating capacity, maximum interunit piping length and maximum installation height difference, please refer to the specifications of the outdoor unit to be connected."]
["","","","","(3) - 240V","(3) - 240V","(3) - Contains fluorinated greenhouse gases"]
["","","","","(4) - Sound values are measured in an anechoic room.","(4) - Sound values are measured in an anechoic room.","(4) - Electric characteristics are only for fan coil unit."]
["","","","","(5) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(5) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","(6) - The sound power level is an absolute value indicating the power which a sound source generates.","(6) - The sound power level is an absolute value indicating the power which a sound source generates."]
["Standard Accessories","Extension auxiliary pipe","","","","2","2"]
["","Installation manual","","","","","1"]
["","Operation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","Heat insulating tape","","","","","2"]