{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":6,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","","FLXS35BAVMB9"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","7.6"]
["Sound pressure level","Cooling","","Nom.","dBA","35"]
["Fan","Air flow rate","Heating","Nom.","m³/min","10.4"]
["Sound pressure level","Heating","","Nom.","dBA","36"]
["Casing","Colour","","","","Almond white"]
["Dimensions","Unit","","Height","mm","490"]
["","","","Width","mm","1050"]
["","","","Depth","mm","200"]
["Weight","Unit","","","kg","16"]
["Fan","Air flow rate","Cooling","High","m³/min","8.6"]
["","","","Low","m³/min","6.6"]
["","","","Silent operation","m³/min","5.6"]
["","","Heating","High","m³/min","12.8"]
["","","","Low","m³/min","8"]
["","","","Silent operation","m³/min","7.2"]
["Sound power level","Cooling","","","dBA","53"]
["","Heating","","","dBA","59"]
["Sound pressure level","Cooling","","High","dBA","38"]
["","","","Low","dBA","32"]
["","","","Silent operation","dBA","29"]
["","Heating","","High","dBA","46"]
["","","","Low","dBA","33"]
["","","","Silent operation","dBA","30"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","OD","mm","9.5"]
["","Drain","","","","18"]
["Control systems","Infrared remote control","","","","ARC433B67"]
["Standard Accessories","Installation manual","","","","1"]
["","Air purification filter","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","Binding band","","","","4"]
["","Operation manual","","","","1"]
["","Heat insulation tube (refrigerant pipe)","","","","8"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Photocatalytic deodorizing filter","","","","1"]
["","Remote control holder","","","","1"]
["","Side cover","","","","2"]
["Power supply","Name","","","","VM"]
["","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]
["","","","","","(4) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected."]