{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":13,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-J3 / RX-K"]
[]
[]
[]
[]
["","","","","FTX20J3V1B / RX20K2V1B","FTX20J3V1B / RX20K5V1B9","FTX20J3V1B / RX20K5V1B","FTX25J3V1B / RX25K2V1B","FTX25J3V1B / RX25K5V1B9","FTX25J3V1B / RX25K5V1B","FTX35J3V1B / RX35K2V1B","FTX35J3V1B / RX35K5V1B9","FTX35J3V1B / RX35K5V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.3","1.3","1.3","1.3","1.3","1.3","1.3"]
["","Max.","","kW","2.6","2.6","2.6","3.0","3.0","3.0","3.8","3.8","3.8"]
["","Nom.","","kW","2.0 (2)","2.0 (2)","2.0 (2)","2.5 (2)","2.5 (2)","2.5 (2)","3.3 (2)","3.3 (2)","3.3 (2)"]
["Space cooling","SEER","","","6.11","6.11","6.11","6.15","6.15","6.15","6.15","6.15","6.15"]
["","Annual energy consumption","","kWh/a","115","115","115","142","143","143","188","188","188"]
["","Capacity","Pdesign","kW","2.00","2.00","2.00","2.50","2.50","2.50","3.30","3.30","3.30"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.20","2.20","2.20","2.40","2.40","2.40","2.80","2.80","2.80"]
["","SCOP/A","","","4.34","4.34","4.34","4.16","4.16","4.16","4.14","4.14","4.14"]
["","Energy efficiency class","","","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["","Annual energy consumption","","kWh/a","711","710","710","809","808","808","947","947","947"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","9.5","9.5","9.5","9.5","9.5","9.5","9.5"]
["","Drain","OD","mm","18","18","18","18","18","18","18","18","18"]
["Nominal efficiency","EER","","","4.09 (1)","4.09 (1)","4.09 (1)","3.55 (1)","3.55 (1)","3.55 (1)","3.21 (1)","3.21 (1)","3.21 (1)"]
["","Annual energy consumption","","kWh","244","244","244","352","352","352","514","514","514"]
["","COP","","","4.24 (1)","4.24 (1)","4.24 (1)","4.06 (1)","4.06 (1)","4.06 (1)","3.76 (1)","3.76 (1)","3.76 (1)"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","2.5 (2)","2.5 (2)","2.5 (2)","2.8 (2)","2.8 (2)","2.8 (2)","3.5 (2)","3.5 (2)","3.5 (2)"]
["","Min.","","kW","1.3","1.3","1.3","1.3","1.3","1.3","1.3","1.3","1.3"]
["","Max.","","kW","3.5","3.5","3.5","4.0","4.0","4.0","4.8","4.8","4.8"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]